Consulta: creatorFacets:"Paes,Juliana L."
Registros recuperados: 8
Data/hora: 09/06/2024 15:41:55

USE OF INOCULUM IN BIODIGESTERS WITH CATTLE MANURE UNDER CONVENTIONAL AND ORGANIC PRODUCTION SYSTEMS
Provedor de dados: Engenharia Agrícola
Autores: Paes,Juliana L.; Alves,Thaís B. S.; Silva,Leonardo D. B. da; Marques,Anieli de S.; Dias,Valentina R. S.
ABSTRACT One way of making livestock farming a more sustainable practice is to raise cattle organically. However, regardless of the production system, there is a generation of residues that can be converted into energy resources using biodigesters. This study aimed to evaluate the addition of inoculum in the anaerobic biodigestion of cattle manure under organic (OPS) and conventional production systems (CPS) in an Indian model biodigester. The physicochemical (pH, EC, TS, VS, DBO, and COD) and microbiological characteristics of the affluent and effluent, as well as the production, potential, and qualitative characteristics of the biogas, were evaluated. CPS showed higher reductions in TS, VS, BOD, and COD than OPS, with the highest effect of biogas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anaerobic biodigestion; Biogas; Starting point; Biofertilizer potential.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200146

Armazenamento de soja em silos tipo bolsa
Provedor de dados: Engenharia Agrícola
Autores: Faroni,Lêda R. A.; Alencar,Ernandes R. de; Paes,Juliana L.; Costa,André R. da; Roma,Rafaela C. C.
Avaliaram-se as principais alterações qualitativas de soja armazenada em silos tipo bolsa e do óleo bruto extraído de soja com teores de água de 17,4% e 13,3%, armazenada em dois silos tipo bolsa, por 180 dias. Realizaram-se amostragens no dia do enchimento das bolsas, aos 30; 90 e 180 dias de armazenamento. Analisaram-se o teor de água, a condutividade elétrica, o percentual de germinação, a massa específica aparente da soja, além do teor de ácidos graxos livres e o índice de peróxido do óleo bruto extraído dela. Os teores de água da soja armazenada úmida e seca mantiveram-se próximos dos valores obtidos no início do período de armazenamento. Observou-se tendência de elevação da condutividade elétrica e decréscimo do percentual de germinação somente na...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Armazenamento hermético; Qualidade; Óleo bruto.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100010

CLASSIFICATION OF ROBUSTA COFFEE FRUITS AT DIFFERENT MATURATION STAGES USING COLORIMETRIC CHARACTERISTICS
Provedor de dados: Engenharia Agrícola
Autores: Costa,Anderson G.; Sousa,Daniela A. G. de; Paes,Juliana L.; Cunha,João P. B.; Oliveira,Marcus V. M. de.
ABSTRACT Coffee growers who produce the robusta species (Conilon) have sought to increase productivity and drink quality by improving production techniques. Artificial vision systems can assist in increasing the efficiency of operations associated with crop management. This study aimed to obtain colorimetric characteristics of robusta coffee fruits at different stages of maturity and use them for classifying fruits from digital images. A digital camera with spectral resolution in the visible was used to acquire images from 60 samples of coffee fruits at the green, cherry, and over-ripe stages of maturity. Colorimetric variables were extracted from the RGB, HIS, and L*a*b* color models and correlated with the physicochemical attributes of the fruits. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Artificial vision systems; Coffea canephora; Principal component analysis.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400518

BIOGAS PRODUCTION FROM DAIRY CATTLE MANURE, UNDER ORGANIC AND CONVENTIONAL PRODUCTION SYSTEMS
Provedor de dados: Engenharia Agrícola
Autores: Matos,Camila F.; Paes,Juliana L.; Pinheiro,Érika F. M.; Campos,David V. B. De.
ABSTRACT The purpose of this study was to evaluate the production of biogas, as well as the biogas production potential resulting from the anaerobic biodigestion of dairy cattle manure under organic (CMOS) and conventional (CMCS) production system. Also, the concentration of thermotolerant coliforms was evaluated after the biodigestion process. Therefore, bench biodigesters prototypes were supplied with CMOS and CMCS for 30 weeks. The experimental design was completely randomized with four repetitions for each treatment. Analysis of total solids (TS), volatile solids (VS), biogas production potential, most probable number (MPN) of thermotolerant coliforms were made. The cumulative biogas production was 6.18 L and 11.15 L, when using the CMOS and CMCS,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anaerobic biodigestion; Biodigester; Agricultural waste.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601081

REACTION KINETICS OF OZONE GAS IN WHEAT FLOUR
Provedor de dados: Engenharia Agrícola
Autores: Paes,Juliana L.; Faroni,Lêda R. A.; Martins,Marcio A.; Cecon,Paulo R.; Heleno,Fernanda F.
ABSTRACT The implementation of the ozonation process in the milling industry to control insect pests and improve wheat flour qualities requires understanding the behavior of ozone during ozonation. Therefore, this study aimed to investigate the reaction kinetics of ozone gas in wheat flour. Wheat flour ozonation at concentrations of 0.54, 1.07, 1.61 and 2.14 mg L−1 was used in a prototype consisting of a cylinder and a mixing system with a helical thread. The iodometric titration method was used to quantify the ozone concentration in the air stream. The reaction kinetics were characterized by determining the saturation time and the decomposition kinetics (decay rate and half-life time). With increasing ozone concentration, less time was required to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ozonation; Saturation; Decay rate; Half-life time.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300520

Aplicação de ozônio contra Sitophilus zeamais e Tribolium castaneum em milho armazenado
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Rozado,Adriano F.; Faroni,Lêda R. A.; Urruchi,Wilfredo M. I.; Guedes,Raul N. C.; Paes,Juliana L.
Neste trabalho a meta principal foi avaliar a suscetibilidade dos adultos de Sitophilus zeamais (Motschulsky) (Coleoptera: Curculionidae) e Tribolium castaneum (Herbst) (Coleoptera: Tenebrionidae) e a qualidade fisiológica dos grãos de milho submetidos ao tratamento com ozônio, em diferentes camadas da massa de grãos, razão pela qual se construíram gaiolas de 3,0 cm de altura e 15,0 cm de diâmetro, em PVC, sendo o fundo e a tampa confeccionados em tecido do tipo organza; as gaiolas foram dispostas em recipientes cilíndricos, também em PVC, com 20 cm de diâmetro, 100 cm de altura e conexões para injeção e exaustão do gás ozônio. Tanto os insetos quanto os grãos de milho foram submetidos a uma atmosfera modificada com 50 mg kg-1 de ozônio injetado a um fluxo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Atmosfera modificada; Insetos; Fumigação.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662008000300009

Diffusion and sorption of allyl isothiocyanate in the process of fumigation of maize
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Paes,Juliana L.; Faroni,Lêda R. A.; Martins,Marcio A.; Dhingra,Onkar D.; Silva,Tales A.
The purpose of this work was to evaluate the transport of allyl isothiocyanate (AITC) by means of the sorption mechanism and the diffusion of AITC through maize grains. The experimental procedure to study the sorption mechanism was conducted by injection of AITC in glass flasks containing the grains. Kinetic models of zero, first and second order were fitted to AITC concentration data, with the purpose of determining the sorption rate (k). For the study of diffusion, a prototype was utilized in which the components are a gas chamber and a cylindrical column in which the grains were stored. At the interval of 110 min, samples in the chamber and in the column were collected, which were immediately injected into the gas chromatograph. In order to determine...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fumigant; Effective diffusion coefficient; Sorption rate.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662011000300011

Influência da temperatura da massa de grãos sobre a toxicidade do ozônio a Tribolium castaneum
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Pereira,Alexandre de M.; Faroni,Lêda R. D'A.; Sousa,Adalberto H. de; Urruchi,Wilfredo I.; Paes,Juliana L.
Considerando que a temperatura da massa de grãos pode influenciar o período de exposição dos fumigantes, desenvolveu-se este trabalho com o propósito de investigar a influência de temperaturas crescentes da massa de grãos (20, 30, 35 e 40 ºC) no período de exposição do ozônio necessário para matar 50 e 95% de insetos adultos de Tribolium castaneum Herbst (Coleoptera: Tenebrionidae). Grãos de milho foram distribuídos em recipientes cilíndricos de PVC com conexões para injeção e exaustão de gás. Os insetos contidos em gaiolas foram colocados na camada mediana da massa de grãos em cada recipiente e estes, por sua vez foram fumigados com ozônio na concentração de 50 ppm. Os tempos letais (TL50 e TL95) para os insetos adultos de T. castaneum foram reduzidos com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ozonização; Pragas de grãos; Armazenamento.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662008000500008