Consulta: creatorFacets:"Sampaio,Silvio C."
Registros recuperados: 39
Data/hora: 09/06/2024 18:17:16

Comportamento das formas de nitrogênio em solo cultivado com milho irrigado com água residuária da suinocultura
Provedor de dados: Engenharia Agrícola
Autores: Sampaio,Silvio C.; Fiori,Marciane G. S.; Opazo,Miguel A. U.; Nóbrega,Lúcia H. P.
A utilização de água residuária com características químicas capazes de complementar ou substituir a adição de fertilizantes químicos tem beneficiado amplamente, tanto em regiões onde ocorre a necessidade de se fazer uso de irrigação, quanto em solos que necessitam de fertilizantes. Porém, uma preocupação ambiental e agronômica deve sempre persistir no uso dessa técnica. Dessa forma, o presente trabalho teve como objetivo avaliar o comportamento das formas de nitrogênio no material percolado e no solo quando cultivado com milho (Zea mays L.) irrigado com água residuária da suinocultura (ARS), em quatro taxas de aplicação (112,5; 225; 337,5 e 450 kg N ha-1) e adubação convencional (AD), em dois níveis (15 e 25 kg N ha-1). O trabalho foi desenvolvido com a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Efluente; Meio ambiente; Contaminação.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100015

Análise operacional de um sistema fotovoltaico de bombeamento de água
Provedor de dados: Engenharia Agrícola
Autores: Kolling,Evandro M.; Souza,Samuel N. M. de; Ricieri,Reinaldo P.; Sampaio,Silvio C.; Dallacort,Rivanildo.
O bombeamento de água é uma das atividades mais difundidas quanto ao emprego da energia solar fotovoltaica. Porém, apesar de se apresentar como alternativa interessante, o alto custo, a baixa eficiência dos sistemas e os projetos inadequados restringem sua aplicação. O uso racional, baseado na utilização mais eficiente de seus equipamentos, está vinculado ao conhecimento do comportamento operacional desses sistemas. No presente trabalho, teve-se o objetivo de avaliar o comportamento de um sistema fotovoltaico de bombeamento de água diretamente acoplado, sob diferentes condições de irradiância solar, por meio da montagem de uma bancada de testes, submetendo-o a diferentes alturas manométricas e determinando-se a vazão fornecida. A análise dos resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irradiância solar; Carga de bombeamento; Vazão do sistema.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300005

Lixiviação de íons em colunas de solo deformado e indeformado
Provedor de dados: Engenharia Agrícola
Autores: Sampaio,Silvio C.; Caovilla,Francielle A.; Opazo,Miguel A. U.; Nóbrega,Lúcia H. P.; Suszek,Morgana; Smanhotto,Adriana.
Neste trabalho, foi avaliada a dinâmica da lixiviação de íons em colunas de solo deformado e indeformado. O solo utilizado era proveniente de área fertirrigada com água residuária da suinocultura diluída em 0%, 25%, 50%, 75% e cultivada com soja. Foram construídas curvas de eluição para nitrato, potássio e condutividade elétrica. De acordo com os resultados obtidos nas colunas de solo deformado, e proporcionalmente aos tratamentos, o nitrato apresentou maior mobilidade, seguido pela concentração de sais totais e do potássio. A metodologia de colunas de solo indeformado não se mostrou adequada, devido, possivelmente, à compactação do solo durante a amostragem e à dificuldade no bloqueio de caminhos preferenciais ao longo de toda a coluna.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água residuária; Meio ambiente; Dinâmica de íons.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100016

IMPLICATIONS FOR PEAK FLOWS OF THE MARRECAS RIVER BASIN DUE TO CHANGES IN THE BRAZILIAN FOREST CODE
Provedor de dados: Engenharia Agrícola
Autores: Aguiar,Wagner de; Sampaio,Silvio C.; Paisani,Julio C.; Reis,Ralpho R. dos.
ABSTRACT Changes in the Brazilian Forest Code (BFC) have soften the criteria for recovery and conservation of permanent preservation areas (PPAs), enhancing processes related to surface runoff. The aim of this study is to understand the effects of changes in PPA classification criteria established by BFC of 2012 to the detriment of BFC from 1965 considering the surface runoff response in the basin draining the upper Marrecas River valley in the flow peaks. The HEC–HMS model was used to simulate flow peaks considering three land-use scenarios, representative of the current use, adapting it to PPAs fitted to the BFC of 1965 and 2012 and seven precipitation return periods. In the proposed scenarios, the use of BFC of 2012, to the detriment of that from 1965,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Surface runoff; Forestry legislation; Hydrological simulation; Land use.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200277

SOIL MESO- AND MACROFAUNA IN TWO SOYBEAN CROPS AFTER SWINE WASTEWATER APPLICATION
Provedor de dados: Engenharia Agrícola
Autores: Maciel,Ana P. C.; Sampaio,Silvio C.; Remor,Marcelo B.; Rosa,Danielle M.; Reis,Ralpho R. Dos.
ABSTRACT Hog raising generates a large amount of residues that is commonly discarded into the soil as fertilizer even with environmental risks. In this context, the aim of this study was to assess the application effects of different doses of swine wastewater (SW) associated with mineral fertilization on the abundance and diversity of organisms of soil meso- and macrofauna in two soybean crops. Treatments consisted of four doses (0, 100, 200, and 300 m3 ha−1) of SW with or without mineral fertilization in two soybean crop, totaling 24 experimental units. Soil meso- and macrofauna were sampled using pitfall traps installed at each plot. Samples were sorted and the organisms were separated and identified. The highest abundances were found between groups of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mineral fertilization; Swine wastewater; Soil fauna.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300556

ADSORPTION OF ATRAZINE BY BIOCHARS PRODUCED FROM BYPRODUCTS OF THE WOOD INDUSTRY
Provedor de dados: Engenharia Agrícola
Autores: Fruehwirth,Marcelo; Sbizzaro,Mariana; Rosa,Danielle M.; Sampaio,Silvio C.; Reis,Ralpho R. dos.
ABSTRACT Atrazine is a herbicide widely used in agriculture; however, because of its toxicity, alternatives are needed to remove this compound from the environment. In this study, we investigated the adsorption process and the atrazine-adsorbing ability of three biochars produced at different pyrolysis temperatures from byproducts of the wood industry. The biochars were characterized by Fourier-transform infrared spectroscopy (FTIR) and scanning electron microscopy (SEM), and their physical characteristics were evaluated by Brunauer-Emmett-Teller (BET) analysis. The biochar pyrolyzed at 350 °C (BM350) adsorbed 26.04% of the herbicide, showing the best performance among the three biochars tested, even though it had the lowest specific surface area (1.467 m2...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water contamination; Isotherm; Functional groups; Kinetics models.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600769

Association of swine wastewater and mineral fertilization on black oat production
Provedor de dados: Engenharia Agrícola
Autores: Herrmann,Daniela da R.; Sampaio,Silvio C.; Castaldelli,Ana P. A.; Tsutsumi,Claudio Y.; Prior,Maritane.
ABSTRACT Swine wastewater (SW) has high organic load, becoming an important source of macro and micronutrients to plants, promoting the improvement of soil quality and development in various cultures. However, when done without agronomic and environmental criteria, it can cause soil problems, nutrient leaching, water resource damage and plant toxicity. The objective of this study was to evaluate the soil chemical properties and the leachate in face of the association of swine wastewater and mineral fertilization (MF) in oat cultivation. An experiment in drainage lysimeter was carried out, using SW applications associated to MF or not, where treatments consisted of doses of 0, 100, 200 and 300 m3ha-1 with the absence or presence of MF, under field...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil fertility; Nutrient leaching; Drainage lysimeters.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500799

Estudo da associação de água residuária de suinocultura e adubação mineral na cultura do milho e no solo
Provedor de dados: Engenharia Agrícola
Autores: Prior,Maritane; Sampaio,Silvio C.; Nóbrega,Lúcia H. P.; Dieter,Jonathan; Costa,Mônica S. S. de M.
RESUMO O uso de água residuária em solo agrícola pode-se caracterizar como uma fonte alternativa de adubação, além de melhorar as condições edáficas do solo devido à matéria orgânica adicionada. Neste contexto, este trabalho teve por objetivo avaliar os efeitos na cultura do milho e em Latossolo Vermelho distroférrico típico, devido à aplicação de água residuária de suinocultura associada com adubação química. No experimento, utilizou-se de cinco doses de ARS (0; 112,5; 225; 337,5 e 450 m3 ha-1) durante o ciclo do milho, combinadas com duas adubações químicas (50 e 75% da dose recomendada), para compor os respectivos tratamentos, com três repetições. Os parâmetros da cultura do milho avaliados foram: produtividade (PROD), altura de plantas (AP), teor de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso de água; Resíduo animal; Valorização agronômica.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400744

Aplicação de água residuária de suinocultura em solo cultivado com soja: cobre e zinco no material escoado e no solo
Provedor de dados: Engenharia Agrícola
Autores: dal Bosco,Tatiane C.; Sampaio,Silvio C.; Opazo,Miguel A. U.; Gomes,Simone D.; Nóbrega,Lúcia H. P.
O objetivo deste trabalho foi avaliar a poluição difusa referente ao cobre e ao zinco no solo e no material de escoamento superficial quando da aplicação de água residuária de suinocultura (ARS) em solo cultivado com soja, sob condição de chuva simulada. O experimento foi instalado em Toledo - PR, sendo aplicadas ao solo cinco taxas de ARS (0; 50; 100; 150 e 200 m³ ha-1 no ciclo), em três repetições por tratamento, divididas em seis aplicações ao longo do ciclo da soja. Foram instaladas calhas coletoras do material escoado e fizeram-se seis simulações de chuva durante o experimento, resultando em seis coletas do material escoado. Ao final do ciclo da soja, foram coletadas amostras de solo em cada uma das parcelas experimentais, em três profundidades, para...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Escoamento superficial; Lixiviação de íons; Reúso de água.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400010

GEOCHEMICAL BACKGROUND IN AN OXISOL
Provedor de dados: Engenharia Agrícola
Autores: Cembranel,Adir S.; Sampaio,Silvio C.; Remor,Marcelo B.; Gotardo,Jackeline T.; Rosa,Pábolla M. Dalla.
ABSTRACT Geochemical background establishment is indispensable to determine the actual state of contamination of soils and sediments. However, no scientific consensus exists regarding the methodology for determining these values. In this context, this study aimed to establish the geochemical background in an Oxisol (Rhodic Hapludox) by means of an integrated method that uses direct and indirect soil analyses to identify the most appropriate calculation methodology. Soil samples were collected in a permanent preservation area of the Cascavel River watershed, PR, Brazil. The elements Cd, Co, Cr, Cu, Fe, K, Mg, Mn, Na, Ni, Pb, and Zn present in soil samples were quantified by flame atomic absorption spectrometry. The use of a permanent preservation area is...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Trace elements; Heavy metals; Sediment; Soil.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300565

Turbidimetry as an alternative method to determine the rating curve of suspended sediments
Provedor de dados: Engenharia Agrícola
Autores: Poletto,Kayla; Sampaio,Silvio C.; Queiroz,Manoel M. F. de; Gomes,Benedito M.; Soncela,Rosimaldo.
Understanding hydrosedimental behavior of a watershed is essential for properly managing and using its hydric resources. The objective of this study was to verify the feasibility of the alternative procedure for the indirect determination of the sediment key curve using a turbidimeter. The research was carried out on the São Francisco Falso River, which is situated in the west of the state of Paraná on the left bank of ITAIPU reservoir. The direct method was applied using a DH-48 sediment suspended sampler. The indirect method consisted of the use of a linigraph and a turbidimeter. Based on the results obtained, it was concluded that the indirect method using a turbidimeter showed to be fully feasible, since it gave a power function-type mathematical model...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Watershed; Hydrosedimentalogy; Agriculture.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300019

Meso e macrofauna de solo cultivado com milho e irrigado com água residuária da suinocultura
Provedor de dados: Engenharia Agrícola
Autores: Castaldelli,Ana P. A; Sampaio,Silvio C.; Tessaro,Dinéia; Herrmann,Daniela da R.; Sorace,Mauren.
RESUMO A utilização da fauna edáfica como bioindicadora de alterações antrópicas e ambientais vem crescendo nos últimos anos. No entanto, ainda são poucos os estudos em longo prazo que relacionam esses organismos com aplicação de resíduos orgânicos no solo. O objetivo deste trabalho foi avaliar, em dois ciclos da cultura do milho, os efeitos da aplicação de diferentes doses e tipos de águas residuárias da suinocultura (ARS) combinadas ou não com adubação mineral sobre a meso e a macrofauna de solo. Quatro doses (0; 100; 200 e 300 m3ha-1) de ARS, tratada em biodigestor no primeiro ano de estudo e bruta no segundo ano, associadas ou não com adubação mineral, foram aplicadas em dois ciclos da cultura de milho, totalizando 24 parcelas experimentais, sendo 12...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fauna edáfica; Reúso de efluente; Dejeto líquido de suíno.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500905

CORN FERTILIZATION USING SWINE WASTEWATER AND SOIL-WATER ENVIRONMENTAL QUALITY
Provedor de dados: Engenharia Agrícola
Autores: Rosa,Danielle M.; Sampaio,Silvio C.; Pereira,Pâmela A. M.; Reis,Ralpho R. Dos; Sbizzaro,Mariana.
ABSTRACT: Soil application of swine wastewater for nutrient cycling may represent a correct destination of these residues and reduction in production costs. However, when applied to soil, such residue may cause environmental impacts. This study aimed to analyze the chemical characteristics of the soil, corn, and leachate after successive swine wastewater applications associated with mineral fertilization. The experiment was developed in drainage lysimeters under field conditions. Wastewater doses applied were 0, 100, 200, and 300 m3 ha−1 with and without mineral fertilization. The results were submitted to analysis of variance and Tukey's test. After nine years of application, a special attention should be taken regarding water quality from a dose of 200...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Liquid residue of swine; No-tillage; Water reuse.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400801

MERCURY IN THE SEDIMENT OF THE UPPER PARNAÍBA RIVER
Provedor de dados: Engenharia Agrícola
Autores: Remor,Marcelo B.; Sampaio,Silvio C.; Rosa,Danielle M.; Model,Kathleen J.; Paloschi,Cristiane L.; Conceição,Fagner G. da.
ABSTRACT The contamination of aquatic environments with chemical trace elements can be evaluated by their accumulation in sediments of the water body. Studies on mercury require the use of exclusive extraction techniques that have relatively high costs when compared to the analysis of other trace elements. This study was conducted aiming at determining the mercury concentration in sediments of the Upper Parnaíba River basin, located in a region of agricultural expansion between the states of Piauí and Maranhão. The sediment was collected at 12 sites in the basin. After drying, the quantification of total mercury was performed by the Zeeman atomic absorption spectrometry coupled to a pyrolysis reactor. Mercury concentrations in sediments of the Parnaíba...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Trace elements; Agricultural frontier; Heavy metal.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500760

ORGANOCLORATED AND ORGANOPHOSPHORUS PESTICIDES IN THE PELOTAS RIVER SEDIMENT
Provedor de dados: Engenharia Agrícola
Autores: Model,Kathleen J.; Sampaio,Silvio C.; Remor,Marcelo B.; Mercante,Erivelto; Boas,Márcio A. Vilas.
ABSTRACT Aquatic sediments are widely used for the evaluation of anthropogenic contamination due to their ability to adsorb particles and contaminants, making them historical environmental archives. Therefore, the objective was to evaluate the contamination of the Pelotas River sediments, at the border between the states of Santa Catarina and Rio Grande do Sul, by organochlorine and organophosphorus compounds, determining the ecological risk. The evaluation was carried out with quarterly sediment collections in 8 points, totalizing four campaigns within one year, with the aid of the Peterson dredger. Among organochlorines, p'p'DDT stands out regarding environmental persistence, representing 53.23% of the contaminated samples, with values varying up to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural pesticides; Disulfoton; P'p'-DDT.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100124

SEASONAL DYNAMICS OF AGRICULTURAL SOIL COVER IN RUNOFF GENERATION
Provedor de dados: Engenharia Agrícola
Autores: Aguiar,Wagner de; Sampaio,Silvio C.; Paisani,Julio C.; Remor,Marcelo B.; Reis,Ralpho R. dos.
ABSTRACT Seasonal changes in agricultural soil use due to agroclimatic conditions affect the water cycle in watersheds. This study aimed to understand the temporal variation of runoff inherent to the seasonal occupation dynamics of the agricultural soil in the basin that drains the upper valley of the Marrecas River, upstream of the urban perimeter of Francisco Beltrão, PR. The effects of runoff were verified through flow peaks simulated by the HEC-HMS model in twelve monthly soil use scenarios, under seven precipitation return periods. The results indicated a strong relationship between bare soil and flow peaks, temporally delimiting April and March as the largest runoff generators and January and August as the smallest ones. The ratio quantified by rates...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Flood; Flow peak; Hydrological simulation; Agricultural soil use.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500592

Reúso de águas residuárias da piscicultura e da suinocultura na irrigação da cultura da alface
Provedor de dados: Engenharia Agrícola
Autores: Baumgartner,Dirceu; Sampaio,Silvio C.; Silva,Tatiana R. da; Teo,Carla R. P. A.; Vilas Boas,Márcio A.
Este trabalho teve o objetivo de avaliar o desenvolvimento, a produção e a qualidade sanitária da cultura da alface irrigada com águas residuárias originadas da suinocultura e da piscicultura. Os tratamentos avaliados foram: T1 - alface irrigada com água de origem subterrânea e adubação suplementar; T2 - alface irrigada com água residuária de viveiro de peixes alimentados com ração; T3 - alface irrigada com água residuária originária de lagoa de estabilização de dejetos de suínos, e T4 - água de lagoa de cultivo de algas, alimentada com resíduo de biodigestor de dejeto de suíno. Os tratamentos não apresentaram diferenças significativas para altura da alface, diâmetro da cabeça, comprimento da raiz, massa da raiz, massa total da planta, massa fresca e massa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Efluente; Irrigação; Lactuca sativa L.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100009

RESIDUE ANALYSIS OF ORGANOCHLORINE AND ORGANOPHOSPHORUS PESTICIDES IN URBAN LAKE SEDIMENTS
Provedor de dados: Engenharia Agrícola
Autores: Cembranel,Adir S.; Frigo,Elisandro P.; Sampaio,Silvio C.; Mercante,Erivelto; Reis,Ralpho R. Dos; Remor,Marcelo B.
ABSTRACT The knowledge of pesticide residual concentrations in the environment is important to understand the threats to the environment and human health, especially when natural resources are used for human consumption. In this context, this study aimed to assess the potential ecological risk and respective sources of sediment contamination by organochlorine and organophosphorus pesticides. The study site was an urban lake located in Cascavel city, western Paraná state, Brazil, where the history of land use and occupation in the urban environment is typically agricultural. Surface sediment samples were collected every three months from April 2010 to June 2013 at five different collection points, totaling 65 samples. Analyses showed that contamination by...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agrochemicals; Ecological risk; Land use and occupation.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601254

STATISTICAL CONTROL OF THE PROCESS APPLIED TO THE MONITORING OF THE WATER QUALITY INDEX
Provedor de dados: Engenharia Agrícola
Autores: Conceição,Ketllin Z. da; Boas,Marcio A. Vilas; Sampaio,Silvio C.; Remor,Marcelo B.; Bonaparte,Danilo I.
ABSTRACT Analyzing the physical-chemical and biological characteristics allows the evaluation of the water quality of a water body. Thus, the objective of this study was to determine the water quality index of the Passaúna and Piraquara rivers, as well as to apply statistical quality control methodologies to evaluate the data resulting from the monitoring of water quality. Therefore, a database with physico-chemical and microbiological parameters of the Passaúna and Piraquara rivers, a watershed of the Iguaçu River, belonging to the cities of Araucária and Piraquara, respectively Paraná, Brazil, was used to carry out the research. The water quality index was determined with the time series and, subsequently, these data were submitted to the statistical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water quality index; Control charts; Capacity of the process.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600951

SWINE WASTEWATER: IMPACTS ON SOIL, PLANT, AND LEACHATE
Provedor de dados: Engenharia Agrícola
Autores: Rosa,Danielle M.; Sampaio,Silvio C.; Pereira,Pâmela A. M.; Mauli,Márcia M.; Reis,Ralpho R. Dos.
ABSTRACT: The use of animal-origin residues as a nutrient source without prior and proper investigations on their positive and negative impacts can affect the quality of agricultural soils and the environment into which they are inserted. In this sense, the aim of this study was to assess the impact of swine wastewater and mineral fertilization application on soil, soybean crop, and leachate characteristics. The experiment was developed in drainage lysimeters under field conditions. The following doses of swine wastewater were applied: 0, 100, 200, and 300 m3 ha−1, both with and without mineral fertilization. Swine wastewater application contributed to increasing soil nutrients; however, a special attention should be paid to Cu+ and Zn+ accumulation, which...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pig slurry; Soil fertility; Leachate; Water reuse.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500928

Construction and calibration of TDR probes for volumetric water content estimation in a Distroferric Red Latosol
Provedor de dados: Engenharia Agrícola
Autores: Soncela,Rosimaldo; Sampaio,Silvio C.; Vilas Boas,Marcio A.; Tavares,Maria H. F.; Smanhotto,Adriana.
The determination of volumetric water content of soils is an important factor in irrigation management. Among the indirect methods for estimating, the time-domain reflectometry (TDR) technique has received a significant attention. Like any other technique, it has advantages and disadvantages, but its greatest disadvantage is the need of calibration and high cost of acquisition. The main goal of this study was to establish a calibration model for the TDR equipment, Trase System Model 6050X1, to estimate the volumetric water content in a Distroferric Red Latosol. The calibration was carried out in a laboratory with disturbed soil samples under study, packed in PVC columns of a volume of 0.0078m³. The TDR probes were handcrafted with three rods and 0.20m...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Apparent dielectric constant; Time-domain reflectometry; Soil water content.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500004

Swine wastewater associated with mineral fertilization on corn crop (Zea mays)
Provedor de dados: Engenharia Agrícola
Autores: Kessler,Nathalie C. H.; Sampaio,Silvio C.; Sorace,Mauren; Lucas,Shaiane D.; Palma,Denise.
This study aimed to evaluate the agronomical and environmental aspects in corn, soil characteristics and leachate resulting from the material combination of swine wastewater and mineral fertilizer in the long run. The experimental area has a history of swine wastewater application for experiments conducted since 2006, this being the seventh crop cycle in the area. Four doses of swine wastewater (0; 100; 200 and 300 m³ ha-1) associated with presence and absence of mineral fertilizer were applied, consisting of eight treatments. The results obtained were subjected to variance analysis and means compared by Tukey test at 5% significance. We conclude that the swine wastewater can be partially used as an alternative fertilizer, since the P and Mn are...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manure; Soil fertility; Water reuse.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300018

Impacts of the application of swine wastewater in percolate and in soil cultivated with soybean
Provedor de dados: Engenharia Agrícola
Autores: Maggi,Cacea F.; Freitas,Paulo S. L. de; Sampaio,Silvio C.; Dieter,Jonathan.
The aim of this study was to evaluate the possible impacts caused in the soil and in the percolate in lysimeters of drainage with application of different rates of swine wastewater (SW) during the cycle of soybean culture and to assess the productivity of it. The experiment was conducted at the Agricultural Engineering Experimental Center of UNIOESTE. The soil was classified as typical Distroferric Red Latosol. There were twenty-four drainage lysimeters in the area in which the soybean was cultivated, cultivar CD 214. Four SW depths (0; 100; 200 and 300 m³ ha-1) were applied to the soil seven days before the sowing in a single application combined with two mineral fertilizations in the sowing (with and without recommended fertilization during sowing), and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lysimeters; Effluent soil pollution.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200007

Atrazine bound residues formation and dissipation in subtropical soil under swine wastewater application
Provedor de dados: Engenharia Agrícola
Autores: Gonçalves,Morgana S.; Sampaio,Silvio C.; Coelho,Silvia R. M.; Suszek,Floriano L.; Cordovil,Claudia M. D. S.
The effects of swine wastewater on atrazine dissipation and formation of bound residues in subtropical clay soil were investigated in this study. The experiment was carried out in laboratory, under room conditions, where samples of Rhodic Hapludox soil received 168.61 mg kg-1 of atrazine and were incubated for 60 days in the following treatments: T1 (sterilized soil + swine wastewater), T2 (sterilized soil + distilled water), T3 (Non sterilized soil + swine wastewater) and T4 (Non sterilized soil + distilled water). The extractable residues and bound residues of atrazine were extracted and analyzed by high performance liquid chromatography. The results showed no effect of swine wastewater on atrazine dissipation. However, the addition of swine wastewater...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Herbicide; Degradation; Sorption; Organic matter.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600017

MERCURY IN THE SEDIMENT OF PELOTAS RIVER BASIN, BRAZIL
Provedor de dados: Engenharia Agrícola
Autores: Remor,Marcelo B.; Sampaio,Silvio C.; Model,Kathleen J.; Falco,Thais D.; Prudente,Victor H. R.
ABSTRACT Many studies have determined the concentration of trace elements in river sediments in Brazil. Notwithstanding, mercury assessments are scarce, especially because of exclusive extraction techniques and expensive analysis techniques. Still, this element is known for its toxicity, persistence, and bioaccumulation, making its presence in the environment an important factor for biota and human health. For this reason, the objective of this study was to determine the mercury concentration in the sediment of the Pelotas River basin, located on the border of the states of Santa Catarina and Rio Grande do Sul. The sediment was collected at eight locations of the Pelotas basin and, after drying, the mercury was quantified by atomic absorption spectrometry...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heavy metal; Trace element; Multivariate statistics.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100117

Movimento de nitrato proveniente de água residuária em colunas de solos
Provedor de dados: Engenharia Agrícola
Autores: Gomes,Eliane R. S.; Sampaio,Silvio C.; Corrêa,Marcus M.; Vilas Boas,Márcio A.; Alves,Luis F. A.; Sobrinho,Teodorico A.
O presente trabalho foi realizado visando à avaliação do movimento do nitrato (N-NO-3) proveniente de águas residuárias de frigorífico, em colunas de solo. No experimento, foram utilizados dois tipos de solo, um de textura argilosa e outro de textura arenosa, ambos corrigidos com calcário, quatro colunas de PVC, de 500 mm de comprimento e 75 mm de diâmetro. Após saturação com CaCl2 0,01 M, foi mantida na parte superior de cada coluna, por meio de frasco de Mariotte, uma lâmina de 100 mm da água residuária, que permitiu uma lâmina total de infiltração correspondente a 2,5 vezes o volume total de poros de cada coluna avaliada. Foi coletado, para cada coluna, um total de 100 amostras do efluente percolado, sendo analisadas 20 amostras com intervalo de cinco...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poluição do solo; Dinâmica de soluto; Lixiviação de sais.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300008

Estado nutricional e qualidade fisiológica de sementes de soja com água residuária da suinocultura
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Passarin,Olga M.; Sampaio,Silvio C.; Rosa,Danielle M.; Reis,Ralpho R. dos; Correa,Marcus M.
Tipo: Info:eu-repo/semantics/other
Ano: 2023
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016010200001

Análise espacial da umidade do solo cultivado com soja sob dois sistemas de manejo
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Zanette,Syonei V.; Sampaio,Silvio C.; Silvestre,Marciane G.; Boas,Márcio A. V.; Uribe-Opazo,Miguel A.; Queiroz,Manoel M. F. de.
Abordaram-se, neste trabalho, aspectos básicos da geoestatística para análise espacial de dados de umidade do solo, com ênfase na análise de semivariograma como metodologia para determinação da dependência espacial. O objetivo consistiu na análise da umidade sob condições de campo, na região de Toledo, PR, em solo argiloso, nas profundidades de 15 e 30cm, sob sistema de manejo plantio direto e preparo convencional do solo; o local da pesquisa foi constituído de duas áreas de 14x14m. Realizou-se, em cada área do experimento, um levantamento por amostragem em uma malha de 64 pontos espaçados 2m, e se utilizou, para análise das amostras, o método convencional (gravimétrico). Os dados foram analisados através da estatística clássica e da geoestatística. Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semivariograma; Geoestatística; Dependência espacial.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662007000300001

Mineral composition and growth of babycorn under swine wastewater combined with chemical fertilization
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Meneghetti,Adriana M.; Nóbrega,Lúcia H. P.; Sampaio,Silvio C.; Ferques,Rafael G.
The objective of this study was to evaluate the application of wastewater from swine manure (ARS) and chemical fertilization on foliar concentrations of macronutrients and micronutrients, and its relationship with the growth of babycorn. An experiment was conducted in completely randomized design with eight treatments and three replications in 4 x 2 factorial arrangement, which consisted of the application of four doses of swine wastewater (0, 40, 80 and 120 kg N ha-1) and two levels of chemical fertilization (0 and 40 kg ha-1). The results indicated that the increase in fertilization using swine wastewater manure resulted in significant differences for babycorn's foliar concentrations of N and P, promoting levels below the adequate for N and K,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays L.; Leaf content nutrients.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662012001100008

Soybean nutritional status and seed physiological quality with swine wastewater
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Passarin,Olga M.; Sampaio,Silvio C.; Rosa,Danielle M.; Reis,Ralpho R. dos; Correa,Marcus M.
ABSTRACT Swine wastewater application is a practice that can become viable in agriculture, for minimizing fertilization costs and improving soil conditions. Therefore, it is essential to establish criteria that define appropriate application doses from the agronomic and environmental perspectives. The objective of this study was to evaluate the effects of swine wastewater doses associated with mineral fertilization on soybean nutritional status and physiological quality of seed. The experiment was conducted in the agricultural year of 2010/2011, using twenty-four drainage lysimeters in randomized block design in 4 x 2 factorial scheme, with four swine wastewater doses (0, 100, 200 and 300 m3 ha-1) applied before sowing, associated with presence and absence...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mineral fertilization; Swine waste; Water reuse.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016000100016

Deslocamento miscível de nitrato e fosfato proveniente de água residuária da suinocultura em colunas de solo
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Anami,Marcelo H.; Sampaio,Silvio C.; Suszek,Morgana; Gomes,Simone D.; Queiroz,Manoel M. F. de.
A fertirrigação com águas residuárias da suinocultura vem sendo muito difundida no País, principalmente na região sul do Brasil, entretanto, o alto potencial poluidor dos dejetos pode tornar-se uma ameaça de contaminação de solos e águas superficiais e subterrâneas se utilizados em quantidades excessivas. Neste trabalho o objetivo principal foi avaliar o processo de lixiviação de íons nitrato e fosfato em colunas de solo, obtendo-se os coeficientes de dispersão hidrodinâmico e o fator de retardamento para a determinação do potencial de contaminação dos lençóis de água subterrâneos. Verificou-se, ainda, o efeito da aplicação de águas residuárias da suinocultura tratada com reatores anaeróbios sobre as propriedades físico-químicas do solo, cujos resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Movimento de íons; Fertirrigação; Contaminação do solo.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662008000100011

Características químicas de solo cultivado com soja e irrigado com água residuária da suinocultura
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Caovilla,Franciele A.; Sampaio,Silvio C.; Smanhotto,Adriana; Nóbrega,Lúcia H. P.; Queiroz,Manoel M. F. de; Gomes,Benedito M.
Neste trabalho se avaliou a distribuição "in situ" de fósforo (P), matéria orgânica (MO), potássio (K), cálcio (Ca), magnésio (Mg), capacidade de troca catiônica (T), alumínio (Al), soma de bases (S), saturação por bases (V) e do pH, em um solo cultivado com soja irrigada com água residuária proveniente da suinocultura (ARS), com níveis de concentração de 0, 25, 50 e 75%. Constituiu-se um esquema fatorial a partir dos quatros níveis de concentração da ARS, das profundidades de 20, 40 e 60 cm com cinco repetições. Os resultados encontrados demonstraram diferenças significativas apenas para P, K e T no perfil do solo. Para todas as características na profundidade de 60 cm, os respectivos níveis de concentração estiveram bastante próximos aos níveis iniciais,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poluição; Lixiviação; Meio ambiente.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662010000700002

Modelo numérico do transporte de água e soluto no solo: I - simulação da distribuição de umidade
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Corrêa,Marcus M.; Martinez,Mauro A.; Costa,Luiz C.; Ruiz,Hugo A.; Corrêa,Marcelo M.; Sampaio,Silvio C.
As equações diferenciais do movimento de água e do transporte de soluto em solo não saturado, considerando-se a existência de extração pela planta, foram resolvidas utilizando a técnica diferenças finitas. Para a implementação do modelo desenvolveu-se um programa em linguagem Delphi, denominado SIMASS-C - SImulação do Movimento de Água e Soluto no Solo, considerando-se a presença de Cultura. O modelo fornece, em diferentes tempos, os valores de umidade, do potencial matricial, do fluxo da água e da concentração de soluto ao longo do perfil do solo. Obtém-se, ainda, como resultados de saída, o crescimento e a densidade das raízes, o índice de área foliar e a evapotranspiração da cultura. Para testar o modelo desenvolvido conduziu-se um experimento em casa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Diferenças finitas; Método iterativo; SIMASS-C.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662006000100003

Uso de manipueira no desenvolvimento vegetativo do milho em ambiente protegido
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Saraiva,Fernanda Z.; Sampaio,Silvio C.; Silvestre,Marciane G.; Queiroz,Manoel M. F. de; Nóbrega,Lúcia H. P.; Gomes,Benedito M.
Avaliaram-se efeitos da água residuária de fecularia tratada por sistema de lagoas, na cultura do milho. A irrigação com água residuária propiciou aumento de todos os parâmetros químicos do solo, proporcional aos respectivos tratamentos como segue: L1E (efluente da lagoa de decantação), L1ED (efluente da lagoa de decantação diluído em 50%), L2E (efluente da primeira lagoa anaeróbia), L2ED (efluente da primeira lagoa anaeróbia diluído em 50%), L3E (efluente da segunda lagoa anaeróbia), L3ED (efluente da segunda lagoa anaeróbia diluído em 50%) e T (testemunha sem adubação, irrigação com água) exceto para o tratamento TA (testemunha com adubação 85 kg ha-1 K2O; 60 kg ha-1 N; 100 kg ha-1 P2O5 e irrigação com água) que também mostrou altos teores dos elementos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água residuária; Fecularia; Reúso; Zea mays L.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662007000100004

Swine farm wastewater and mineral fertilization in corn cultivation
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Pereira,Pâmela A. M.; Sampaio,Silvio C.; Reis,Ralpho R. dos; Rosa,Danielle M.; Correa,Marcus M.
ABSTRACT In the long run, swine wastewater can provide benefits to the soil-plant relationship, when its use is planned and the potential environmental impacts are monitored. The objective of this study was to investigate the effects of continuous application of swine wastewater, associated with mineral fertilization, after six years of management in no-tillage and crop rotation (14 production cycles), on the chemical conditions of the soil and the corn crop. The doses of wastewater were 0, 100, 200, 300 m3 ha-1 during the cycle. The effects of the association between mineral fertilization at sowing and swine wastewater were evaluated simultaneously. Swine wastewater at the dose of 100 m3 ha-1 promoted availability and absorption of P, K+, Mg2+ and Zn2+...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertigation; Water reuse; Swine waste.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016000100049

Perda de carga contínua em tubulações conduzindo água residuária da suinocultura
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Sampaio,Silvio C.; Denículi,Wilson; Oliveira,Rubens A.; Silva,Demétrius D. da; Matos,Antônio T.; Martinez,Mauro A.
O presente trabalho foi desenvolvido com o objetivo de definir e avaliar modelos matemáticos que estimem a perda de carga contínua em tubulações de aço zincado, ferro galvanizado e PVC, nos diâmetros comerciais 2 a 6 polegadas. Utilizou-se como fluido escoante a água e água residuária proveniente da suinocultura, nas concentrações de 0,98; 2,08; 4,73; 7,69 e 8,56%. Os resultados mostraram que os métodos que estimam a perda de carga baseados na equação Universal e relacionam o fator de atrito às características de escoamento, não apresentaram bons ajustes, principalmente quando se utilizou o Número de Reynolds Generalizado. As equações empíricas, propostas neste trabalho, em que se utilizam as metodologias de Duffy &amp;amp; Titchener e Hazen-Williams...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Perda de carga; Fluido não newtoniano; Efluente.
Ano: 2001
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662001000300005

Nonpoint source pollution by swine farming wastewater in bean crop
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Doblinski,André F.; Sampaio,Silvio C.; Silva,Vanderlei R. da; Nóbrega,Lúcia H. P.; Gomes,Simone D.; Dal Bosco,Tatiane C.
In order to verify the environmental impact of the application of swine farming wastewater in bean crop, an experiment was set up in the Experimental Farm of PUCPR - Toledo, PR, Brazil. Runoff and soil samples were collected at the end of the experiment. Four wastewater treatments were utilized during the experiment (50, 100, 150 and 200 m³ ha-1) and the without wastewater as the control. The results demonstrate that (i) the amounts of potassium, phosphorus, and nitrogen in runoff are exponential, (ii) that phosphorus has a seven-fold polluting potential compared to potassium and three-fold compared to nitrogen, and (iii) that the mobility of potassium in the soil profile is the largest, followed by those of nitrogen and phosphorus.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water reuse; Runoff; Environmental pollution.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662010000100012

Reforested soil under drip irrigation with treated wastewater from poultry slaughterhouse
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Araujo,Izabela R. C.; Sampaio,Silvio C.; Paz-Gonzalez,Antonio; Vilas-Boas,Márcio A.; Gonçalves Junior,Affonso C.; Szekut,Flávio D.
ABSTRACT The disposal of treated effluents on soil is the main final use of wastewater in Brazil. Although this practice can promote improvements of some soil attributes, there is a need for monitoring in order to ensure that potential environmental impacts are not harmful. Thus, the purpose of this study was to evaluate the effects of treated effluent from a poultry slaughterhouse on the chemical attributes of an Oxisols, in Matelândia-PR, Brazil under drip irrigation. The soil attributes P, K, Fe, Cu, Zn, Mn, pH in CaCl2, H + Al, Al, Ca, Mg, cation exchange capacity (CEC), and percent base saturation (V) were evaluated under four effluent application rates, 0, 100, 200 and 300 m³ ha-1 d-1 with treated effluents on three successive sampling dates. As main...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Forestry production; Eucalyptus; Oxisols.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662019000600439

Equação de Hazen-Williams corrigida para água residuária proveniente da suinocultura
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Sampaio,Silvio C.; Cilene,Kátia; Boas,Márcio A. Vilas; Queiroz,Manoel M. F. de; Gomes,Benedito M.; Fazolo,Ajadir.
O objetivo do trabalho foi avaliar a perda de carga em tubulações comerciais de aço zincado, ferro galvanizado e PVC, com diferentes diâmetros, com o intuito de determinar fatores de correção para a equação de Hazen-Williams em função da concentração de sólidos totais, em águas residuárias oriundas da suinocultura. Os resultados mostraram que a perda de carga possui comportamento linear em função da concentração de sólidos totais da água residuária proveniente da suinocultura; as perdas de carga determinadas a partir dos fatores de correção parcial e global, apresentaram superestimativa e subestimativa média de 0,7 e 13%, respectivamente.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso de água; Irrigação; Hidráulica.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662007000100001