Consulta: creatorFacets:"Trugilho,Paulo Fernando"
Registros recuperados: 7
Data/hora: 09/06/2024 18:42:36

Mass and energy balance of the carbonization of babassu nutshell as affected by temperature
Provedor de dados: 86
Autores: Protásio,Thiago de Paula; Trugilho,Paulo Fernando; Napoli,Alfredo; Silva,Marcela Gomes da; Couto,Allan Motta.
The objective of this work was to evaluate the carbonization yield of babassu nutshell as affected by final temperature, as well as the energy losses involved in the process. Three layers constituting the babassu nut, that is, the epicarp, mesocarp and endocarp, were used together. The material was carbonized, considering the following final temperatures: 450, 550, 650, 750, and 850ºC. The following were evaluated: energy and charcoal yields, pyroligneous liquid, non-condensable gases, and fixed carbon. The use of babassu nutshell can be highly feasible for charcoal production. The yield of charcoal from babassu nutshell carbonization was higher than that reported in the literature for Eucalyptus wood carbonization, considering the final temperature of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Alternative biomass; Charcoal; Iron industry; Renewable energy.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2014000300189

Comparação de métodos de determinação da densidade básica em Madeira
Provedor de dados: 36
Autores: Trugilho,Paulo Fernando; Silva,Dimas Agostinho da; Frazão,Francisco Juvenal Lima; Matos,Jorge Luis Monteiro de.
O presente trabalho visou o estudo comparativo de 6 métodos propostos para a determinação da densidade básica em madeira e ainda, o efeito de 3 dimensões dos corpos de prova nos métodos. Para tal empregou-se distintamente cerne e alburno da espécie Hymenaea cobaril L. (jatobá) em corpos de provas nas dimensões 2 x 2 x 1 com (D1), 2 x 2 x 3 com (D2) e 2 x 2 x 5 cm (D3). Os métodos analisados foram: a) método de imersão-baseado na variação do peso do líquido (M1); b) o método de medição direta do volume por paquímetro (M2); c) método de imersão-baseado na variação do peso da amostra (M3); d) método de medição direta do volume por cilindro graduado-corpo de prova imerso em areia (M4); e) método de máximo teor de umidade (M5) e f) método de medição direta do...
Tipo: Info:eu-repo/semantics/article
Ano: 1990
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0044-59671990000100307

Características de crescimento, composição química, física e estimativa de massa seca de madeira em clones e espécies de Eucalyptus jovens
Provedor de dados: 65
Autores: Trugilho,Paulo Fernando; Goulart,Selma Lopes; Assis,Claudinéia Olímpia de; Couto,Fernanda Bueno Sarro; Alves,Isabel Cristina Nogueira; Protásio,Thiago de Paula; Napoli,Alfredo.
O objetivo deste trabalho foi avaliar o efeito do material genético, clones e espécies, e da classe de diâmetro nas características de crescimento, composição química, densidade básica e a estimativa de massa seca de madeira. Foram avaliados quatro clones e cinco espécies, aos quatro anos de idade, de Eucalyptus procedentes da empresa RIMA Industrial S.A. Foram avaliadas cinco árvores por clone e espécie em três e quatro classes diamétricas, respectivamente. Avaliaram-se as características individuais de crescimento da árvore, a densidade básica, a estimativa de massa seca, o teor de lignina, extrativos totais, holocelulose e cinzas. O volume, com e sem casca, e a estimativa de massa seca apresentaram efeito significativo de material genético (clone e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Qualidade; Madeira jovem; Eucalipto.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782015000400661

Use of sawdust Eucalyptus sp. in the preparation of activated carbons
Provedor de dados: 64
Autores: Couto,Gabriela Martucci; Dessimoni,Anelise Lima de Abreu; Bianchi,Maria Lúcia; Perígolo,Deise Morone; Trugilho,Paulo Fernando.
Wood sawdust is a solid residue, generated in the timber industry, which is of no profitable use and can cause serious environmental problems if disposed inadequately. The aim of this study was to use the eucalyptus sawdust in the preparation of activated carbons AC) and test them as adsorbents of methylene blue (MB) and phenol, representative pollutants from aqueous effluents of various industries. The eucalyptus sawdust was characterized by instrumental analysis such as elementary analysis (CHNS-O), thermogravimetric analysis (TGA), infrared spectroscopy (FTIR) and scanning electron microscopy (SEM). The activated carbons were prepared by physical activation with carbon dioxide AC_CO2, (10º C min-1, 850º C, 1h) and by chemical activation with potassium...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agro-industrial residues; Adsorbents; Pollutants.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542012000100009

Densidade básica e estimativa de massa seca e de lignina na madeira em espécies de Eucalyptus
Provedor de dados: 64
Autores: Trugilho,Paulo Fernando.
Objetivou-se, no presente trabalho, usar três diferentes formas para estimar a densidade básica da madeira, visando a obtenção da estimativa de massa seca e a massa de lignina na madeira em nove espécies de Eucalyptus, em diferentes idades. Foram usadas três formas de estimativa da densidade básica da madeira, ou seja, em um único ponto no tronco (1,3 m de altura do solo), a média ponderada pelo volume e a média aritmética. Essas estimativas foram usadas para a determinação da massa seca e de lignina na madeira. Os resultados indicam que o Eucalyptus grandis W.Hill. (EG), aos quatro anos, e o híbrido (HB), nas demais idades, foram as espécies que se destacaram no incremento volumétrico. O efeito da forma de estimativa somente foi significativo para a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Densidade básica; Madeira; Eucalyptus.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542009000500005

Quality and energetic evaluation of the charcoal made of babassu nut residues used in the steel industry
Provedor de dados: 64
Autores: Protásio,Thiago de Paula; Trugilho,Paulo Fernando; Mirmehdi,Seyedmohammad; Silva,Marcela Gomes da.
Brazil is the only country in the world that uses large scale charcoal in steel-making blast furnaces. Meantime, the monoculture plantations of Eucalyptus are not able to meet the demand for charcoal from the steel industries.Therefore, research is necessary, in order to use lignocellulosic residues for the production of charcoal with technological properties which are suitable for the reduction of iron ore. Given the above, the objective of this study was to evaluate the quality of charcoal which was made with babassu nut shell and designed for utilization in the steel industry in the function of the final carbonization temperature. All three layers of babassu nut shell (epicarp, mesocarp and endocarp) were used together. The initial temperature of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Alternative biomass; Renewable energy; Bio-reducer; Carbonization.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542014000500003

Thermal decomposition of torrefied and carbonized briquettes of residues from coffee grain processing
Provedor de dados: 64
Autores: Protásio,Thiago de Paula; Melo,Isabel Cristina Nogueira Alves de; Guimarães Junior,Mario; Mendes,Rafael Farinassi; Trugilho,Paulo Fernando.
The use of biomass has been recognized as a potential renewable energy and an alternative substitute that contributes to the decrease of fossil fuels consumption. Therefore, this research aimed to analyze the thermal behavior of briquettes made of residues from coffee grain processing in different conditions: in natura, torrefied and carbonized. Eucalyptus sawdust was used for comparison. The briquettes were carbonized considering final temperature of 450° C (kept for 30 min). The briquettes torrefaction was performed in an electric oven (muffle) using two heating rates until 250° C (kept 60 min). The thermal-gravimetric analysis was made in nitrogen atmosphere until the temperature of 600° C. The contents of fixed carbon and volatile matter of the fuels...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solid biofuels; Residual biomass; Coffee plantations; Stability.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542013000300004