Consulta: creatorFacets:"Viana,Edna M. de F."
Registros recuperados: 1
Data/hora: 10/06/2024 00:33:34

Abrasive effects of sediments on impellers of pumps used for catching raw water
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Serrano,Rodrigo O. P.; Castro,Ana L. P. de; Rico,Edwin A. M.; Pinto,Maria A.; Viana,Edna M. de F.; Martinez,Carlos B.
ABSTRACT This study presents an analysis of the abrasive effects of sediments from the bed of the Acre River, Brazil, on the wear of three different ferrous materials employed in the manufacture of impellers of centrifuge pumps used to catch raw water. In order to evaluate the abrasive wear and specific wear coefficient (k) as a function of sediment concentration, tests were conducted in samples of SAE 8620 steel, nodular cast iron and gray cast iron by using a rotary-ball abrasion meter. These tests employed abrasive slurry with concentration of 1, 2, 3, 5 and 10 g L-1 of sediments in distilled water. The volume of worn material as a function of the relative velocity of water flow in relation to the impeller blades was mathematically estimated. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Abrasive wear; Micro abrasion; Sediment concentration.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662018000900591