Consulta: creatorFacets:"Wenzhoefer, Frank"
Registros recuperados: 2
Data/hora: 09/06/2024 03:50:55

Diversity and distribution of cold-seep fauna associated with different geological and environmental settings at mud volcanoes and pockmarks of the Nile Deep-Sea Fan
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Ritt, Benedicte; Pierre, Catherine; Gauthier, Olivier; Wenzhoefer, Frank; Boetius, Antje; Sarrazin, Jozee.
The Nile Deep-Sea Fan (NDSF) is located on the passive continental margin off Egypt and is characterized by the occurrence of active fluid seepage such as brine lakes, pockmarks and mud volcanoes. This study characterizes the structure of faunal assemblages of such active seepage systems of the NDSF. Benthic communities associated with reduced, sulphidic microhabitats such as sediments and carbonate crusts were sampled by remotely operated vehicles during two cruises in 2006 (BIONIL) and 2007 (MEDECO). Environmental conditions and biological factors including family-level faunal composition, density and diversity were measured at local and regional scales. Significant differences were detected at different spatial scales: (1) the fauna of reduced habitats...
Tipo: Text
Ano: 2011
URL: http://archimer.ifremer.fr/doc/00037/14798/12212.pdf

An Assessment of the Precision and Confidence of Aquatic Eddy Correlation Measurements
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Donis, Daphne; Holtappels, Moritz; Noss, Christian; Cathalot, Cecile; Hancke, Kasper; Polsenaere, Pierre; Wenzhoefer, Frank; Lorke, Andreas; Meysman, Filip J. R.; Glud, Ronnie N.; Mcginnis, Daniel F.
The quantification of benthic fluxes with the aquatic eddy correlation (EC) technique is based on simultaneous measurement of the current velocity and a targeted bottom water parameter (e.g., O2, temperature). High-frequency measurements (64 Hz) are performed at a single point above the seafloor using an acoustic Doppler velocimeter (ADV) and a fast-responding sensor. The advantages of aquatic EC technique are that 1) it is noninvasive, 2) it integrates fluxes over a large area, and 3) it accounts for in situ hydrodynamics. The aquatic EC has gained acceptance as a powerful technique; however, an accurate assessment of the errors introduced by the spatial alignment of velocity and water constituent measurements and by their different response times is...
Tipo: Text
Palavras-chave: Turbulence; Boundary layer; Fluxes; Instrumentation/sensors; Optimization; Experimental design.
Ano: 2015
URL: https://archimer.ifremer.fr/doc/00275/38577/37102.pdf