Consulta: subjectFacets:"Desulfurobacterium crinifex"
Registros recuperados: 1
Data/hora: 17/06/2024 20:16:12

Desulfurobacterium crinifex sp.nov., a novel thermophilic, pinkish-streamer forming, chemolithoautotrophic bacterium isolated from a Juan de Fuca Ridge hydrothermal vent and amendment of the genus Desulfurobacterium
Provedor de dados: 5
Autores: Alain, Karine; Rolland, Sophie; Crassous, Philippe; Lesongeur, Francoise; Zbinden, Magali; Le Gall, Christian; Godfroy, Anne; Page, Antoine; Juniper, S Kim; Cambon-bonavita, Marie-anne; Duchiron, Francis; Querellou, Joel.
A novel thermophilic, chemolithoautotrophic T bacterium, designated as NE1206(T), was isolated from a Juan de Fuca Ridge hydrothermal vent sample (tubes of the annelid polychaete Paralvinella sulfincola attached to small pieces of hydrothermal chimney). The cells were rod-shaped (1.2-3.5x0.4-0.7 mum), occurring as single motile rods or forming macroscopic aggregates visible as pinkish to brownish streamers. The new isolate was anaerobic. It grew between 50 and 70 degreesC (optimum 60-65 degreesC doubling time approximately 1 h 15 min at 60 degreesC), between pH 5.0 and 7.5 (optimum pH around 6.0-6.5) and at sea salts concentrations between 20 and 40 g l(-1) (optimum 30 g l(-1)). Cells grew chemolithoautotrophically in an H-2/CO2 atmosphere (80/20, v/v; 200...
Tipo: Text
Palavras-chave: Thermophile; Nitrate reducing; Lithotroph; Desulfurobacterium crinifex; Deep sea hydrothermal vent; Cell networks.
Ano: 2003
URL: https://archimer.ifremer.fr/doc/2003/publication-663.pdf