Consulta: subjectFacets:"Drainage water (see Percolation water)"
Registros recuperados: 8
Data/hora: 17/06/2024 04:31:19

Water temperature in irrigation return flow from the Upper Snake Rock watershed
Provedor de dados: 18
Autores: Bjorneberg, D.L.
Water returning to a river from an irrigated watershed could increase the water temperature in the river. The objective of this study was to compare the temperature of irrigation return flow water with the temperature of the diverted irrigation water. Water temperature was measured weekly in the main irrigation canal, 24 return flow streams and one ephemeral stream from 2005 to 2008 in the Upper Snake Rock (USR) watershed. The USR is an 82,000 ha watershed in southern Idaho, USA with about 60% of the area surface irrigated and the remaining area sprinkler irrigated. Median annual water temperatures in irrigation return flow streams were not greater than the water diverted from the river, suggesting that water flowing through the canal system and furrow...
Tipo: Article
Palavras-chave: Drainage water (see Percolation water); Water.
Ano: 2015
URL: http://eprints.nwisrl.ars.usda.gov/1594/1/1552.pdf

Ponding Surface Drainage Water for Sediment and Phosphorus Removal
Provedor de dados: 18
Autores: Brown, M.J.; Bondurant, J.A.; Brockway, C.E.
Tipo: Article
Palavras-chave: Drainage water (see Percolation water); Sediment; Mass Import - autoclassified (may be erroneous).
Ano: 1981
URL: http://eprints.nwisrl.ars.usda.gov/381/1/475.pdf

Microbiological Quality of Surface Drainage Water from Three Small Irrigated Watersheds in Southern Idaho
Provedor de dados: 18
Autores: Smith, J.H.; Douglas, C.L.
Tipo: Article
Palavras-chave: Drainage water (see Percolation water); Mass Import - autoclassified (may be erroneous).
Ano: 1973
URL: http://eprints.nwisrl.ars.usda.gov/230/1/242.pdf

Sediment in Irrigation and Drainage Waters and Sediment Inputs and Outputs for Two Large Tracts in Southern Idaho
Provedor de dados: 18
Autores: Brown, M.J.; Carter, D.L.; Bondurant, J.A.
Tipo: Article
Palavras-chave: Drainage water (see Percolation water); Sediment; Mass Import - autoclassified (may be erroneous).
Ano: 1974
URL: http://eprints.nwisrl.ars.usda.gov/258/1/285.pdf

Microbiological Quality of Subsurface Drainage Water From Irrigated Agricultural Land
Provedor de dados: 18
Autores: Smith, J.H.; Douglas, C.L.; Bondurant, J.A.
Tipo: Article
Palavras-chave: Drainage water (see Percolation water); Mass Import - autoclassified (may be erroneous).
Ano: 1972
URL: http://eprints.nwisrl.ars.usda.gov/207/1/194.pdf

Phosphorus Associated With Sediments in Irrigation and Drainage Waters for Two Large Tracts in Southern Idaho
Provedor de dados: 18
Autores: Carter, D.L.; Brown, M.J.; Robbins, C.W.; Bondurant, J.A.
Tipo: Article
Palavras-chave: Drainage water (see Percolation water); Sediment; Mass Import - autoclassified (may be erroneous).
Ano: 1974
URL: http://eprints.nwisrl.ars.usda.gov/259/1/286.pdf

Design and calibration of percolation samplers for measuring polyacrylamide-amended furrow-irrigation effects on drainage water quality
Provedor de dados: 18
Autores: Lentz, Rodrick D.; Sojka, Robert E.; Kincaid, Dennis C.
Tipo: Conference or Workshop Item
Palavras-chave: Drainage water (see Percolation water); Polyacrylamide; Percolation water; Percolation sampler; Polyacrylamide; Drainage water (see Percolation water); Percolation water; Polyacrylamide; Research methodology; Mass Import - autoclassified (may be erroneous).
Ano: 1998
URL: http://eprints.nwisrl.ars.usda.gov/860/1/959.pdf

Assessment of Phosphorus Retention in   Irrigation Laterals
Provedor de dados: 18
Autores: Ippolito, J.A.; Nelson, N.O.
Irrigation  laterals  transport  irrigation  return  flow,  including  water,  sediment, and dissolved nutrients, such as phosphorus (P), back to surface water bodies. Phosphorus transformations during transport can affect both P bioavailability and the best management practices selected to minimize P inputs to waters of the United States. The objective of this study  was  to  determine  P  retention  in  three  irrigation  laterals.  Soluble  reactive  P  (SRP) concentrations in lateral waters were increased from 0.08 to 0.25 mg L -1  (0.08 to 0.25 ppm) by constantly injecting a phosphate (PO4) solution for 2.5 hours. Bromide (Br) was used as a conservative tracer to determine dilution effects. Water was sampled at 10-minute intervals, beginning 30...
Tipo: Article
Palavras-chave: Drainage water (see Percolation water); Nutrients.
Ano: 2013
URL: http://eprints.nwisrl.ars.usda.gov/1513/1/1477.pdf