Consulta: subjectFacets:"Organic loading rate"
Registros recuperados: 2
Data/hora: 09/06/2024 02:58:56

Effect of temperature on the anaerobic digestion of palm oil mill effluent
Provedor de dados: 69
Autores: Choorit,Wanna; Wisarnwan,Pornpan.
Two continuous stirred tank reactors (CSTRs) each fed with palm oil mill effluent (POME), operated at 37ºC and 55ºC, respectively, were investigated for their performance under varies organic loading rates (OLRs). The 37ºC reactor operated successfully at a maximum OLR of 12.25 g[COD]/L/day and a hydraulic retention time (HRT) of 7 days. The 55ºC reactor operated successfully at the higher loading rate of 17.01 g[COD]/L/day and had a HRT of 5 days. The 37ºC reactor achieved a 71.10% reduction of chemical oxygen demand (COD), a biogas production rate of 3.73 L of gas/L[reactor]/day containing 71.04% methane, whereas the 55ºC reactor achieved a 70.32% reduction of COD, a biogas production rate of 4.66 L of gas/L[reactor]/day containing 69.53% methane. An OLR...
Tipo: Journal article
Palavras-chave: Hydraulic retention times; Mesophilic reactor; Methane; Organic loading rate; Temperature variations; Thermophilic reactor; Volatile fatty acids.
Ano: 2007
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0717-34582007000300005

Biomethane production from vinasse in upflow anaerobic sludge blanket reactors inoculated with granular sludge
Provedor de dados: 58
Autores: Barros,Valciney Gomes de; Duda,Rose Maria; Oliveira,Roberto Alves de.
ABSTRACT The main objective of this study was to evaluate the anaerobic conversion of vinasse into biomethane with gradual increase in organic loading rate (OLR) in two upflow anaerobic sludge blanket (UASB) reactors, R1 and R2, with volumes of 40.5 and 21.5 L in the mesophilic temperature range. The UASB reactors were operated for 230 days with a hydraulic detection time (HDT) of 2.8 d (R1) and 2.8-1.8 d (R2). The OLR values applied in the reactors were 0.2-7.5 g totalCOD (L d)−1 in R1 and 0.2-11.5 g totalCOD (L d)−1 in R2. The average total chemical oxygen demand (totalCOD) removal efficiencies ranged from 49% to 82% and the average conversion efficiencies of the removed totalCOD into methane were 48-58% in R1 and 39-65% in R2. The effluent recirculation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogas; Mesophilic anaerobic treatment; Methane; Organic loading rate; Startup.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822016000300628