Consulta: subjectFacets:"Pineapple silage"
Registros recuperados: 1
Data/hora: 10/06/2024 18:05:30

Particle passage kinetics and neutral detergent fiber degradability of silage of pineapple waste (aerial parts) under different packing densities
Provedor de dados: 96
Autores: Caetano,Graciele Araújo de Oliveira; Villela,Severino Delmar Junqueira; Oliveira,Margarida Maria Nascimento Figueiredo de; Leonel,Fernando de Paula; Tamy,Wagner Pessanha.
The objective of this study was to determine the kinetics of in situ degradability parameters of the dry matter (DM) and neutral detergent fiber (NDF) and the passage of materials originating from the ensilage of the waste from pineapple cultivation (aerial parts). The four treatments utilized were silage of pineapple waste compacted at 600, 700, 900 and 1000 kg/m³. After ensiling the material from the pineapple cultivation, the particle-transit and rumen-degradation kinetics were analyzed. For the analysis of particle transit, chromium was utilized as a marker to mark the fiber. Passage rates were determined by retrieving the markers in the feces of the animals. In the degradation assay, samples were incubated in nylon bags for 0, 6, 18, 48 and 96 hours....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compaction; Mean retention time in the rumen; Pineapple silage; Rumen fill.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-35982014000100008