Consulta: subjectFacets:"Pressurized irrigation"
Registros recuperados: 2
Data/hora: 09/06/2024 11:21:17

Análisis costo - beneficio de la ampliacíón del distrito de riego No. 110 "Río Verde - Progreso, Oax.".
Provedor de dados: Depósito Institucional Abierto de Documentos Digitales del Colegio de Postgraduados (COLPOS DIGITAL )
Autores: Ramos Solano, José Filiberto.
Se presenta una propuesta de ampliación del Distrito de Riego 110 “Río Verde – Progreso, Oax.”, como una de las acciones complementarias del proyecto de generación de energía eléctrica “Paso de la Reyna”, impulsada por el Gobierno Federal a través de la Comisión Federal de Electricidad. El proyecto de inversión considera incorporar la superficie dominada por la COTA 35, que parte de la base de la cortina de la presa de regulación que se ubicará aguas abajo de la presa “Paso de la Reyna”, y que suman 8,566 hectáreas. Para fines de análisis, el proyecto de ampliación se dividió en dos partes: a) dos líneas principales de conducción, una a cada margen del Río Verde, que suman una longitud total de 56,307 m y que dominan toda la superficie de ampliación...
Palavras-chave: Modernización del riego; Paso de la Reyna; Riego presurizado; Análisis costo-beneficio; Irrigation improvement; Pressurized irrigation; Cost-benefit analysis; Hidrociencias; Maestría Tecnológica.
Ano: 2013
URL: http://hdl.handle.net/10521/1946

Numerical study of upstream disturbances on the performance of electromagnetic and ultrasonic flowmeters
Provedor de dados: Scientia Agricola
Autores: Palau,Carmen Virginia; Bomfim,Guilherme Vieira do; Azevedo,Benito Moreira de; Peralta,Iban Balbastre.
ABSTRACT Electromagnetic and ultrasonic flowmeters are high precision devices that can measure the water flow in pressurized irrigation networks. In these networks, the inadequate installation distance of flow control valves generates upstream disturbances which will increase measurement errors and reduce the accuracy of the equipment. Therefore, estimating these errors is important to establishing the correct installation distance of the hydraulic accessories and to ensuring the metrological reliability of the flowmeters. This work proposes a numerical study using Computational Fluid Dynamics to evaluate water flow behavior in pipes and estimate measurement errors caused by gate and butterfly valves in installation configurations found at pressurized...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: CFD; Pressurized irrigation; Water flowmeter; Water supply network.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162020000401602