Consulta: subjectFacets:"Radiometers"
Registros recuperados: 2
Data/hora: 03/06/2024 09:24:44

Etude des transports de matieres en suspension en Manche par l''emploi de l'imagerie CZCS
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Thomas, Y.
The suspended matter distribution in Channel surface waters during 1981 have been obtained by the interpretation of radiometer recording (Coastal zone Color Scanner working on Nimbus 7 satellite). After imagery calibration and calculation of suspended matter concentration using algorithm from in situ measurements, the maps interpretation allows the study of: (1) resuspension of infratidal fluvial particles by swells and tides; (2) characterizing of intertidal zone given estuarine material by erosion; (3) determination of river plume limits with regard to Seine flow rate; (4) calculation and modeling of solid load; (5) estimation of suspended particles masses and volumes to strike the balance; (6) differentiation of hydrobiological behaviors in Western and...
Tipo: Text
Palavras-chave: Turbidity; Coastal zone; Estuarine front; River plumes; Zonal distribution; Estuarine dynamics; Radiometers; Remote sensing; Suspended particulate matter; Particle motion.
Ano: 1985
URL: http://archimer.ifremer.fr/doc/1985/acte-1280.pdf

Aspectos generales sobre la estructura térmica superficial del mar, de la zona comprendida entre el golfo de Penas y la boca occidental del estrecho de Magallanes
Provedor de dados: Ocean Docs: e-repository of  publications
Autores: Boré, D.; Barbieri, M.A.; Catasti, V.
This study was carried out within the Project Cimar-Fiordo 2. The general objective was to describe the sea surface temperature in the zone between 46º LS and 52º LS, and from the 73º 52’ LW to the 76º 30’ LW, considering the channel and fjord zone. The analysis was based on satellite images of sea surface temperature. The images used came from the AVHRR radiometer of the NOAA satellite, from the year 1995 to 1998.   The cartographic representation and the analysis of the seasonal variability of the sea surface temperature was made using the software of the Geographical Information System (GIS), named IDRISI. The zone was with clouds during all the period of study, mainly in autumn. With the available images it was possible to observe a big difference...
Tipo: Journal Contribution
Palavras-chave: Water temperature; Fjords; GIS; Satellite sensing; Radiometers; Surface temperature; Sea water; Thermal structure; Water temperature; Fjords; Radiometers; Sea water.
Ano: 2001
URL: http://hdl.handle.net/1834/1578