Consulta: subjectFacets:"Seagass"
Registros recuperados: 1
Data/hora: 03/06/2024 17:00:44

An underwater tracking system for mapping marine communities: an application to Posidonia oceanica
Provedor de dados: 5
Autores: Sgorbini, S; Peirano, A; Cocito, S; Morgigni, M.
The GPS intelligent buoy is a pot-table underwater tracking system consisting of four buoys and one pinger. The pinger was mounted on an underwater vehicle driven by a Scuba diver and used to map the limits of a Posidonia oceanica meadow. To test the accuracy of the method the system was tried out on different types of limits and on healthy and regressed part of the meadow from 2 to 25 m of depth. The time of track acquisition (1 point per second), the recording speed (1 km h(-1)) and the mapping scale (more than 1:500) indicated that the proposed method may be successfully integrated with conventional systems for mapping marine communities. (C) 2002 Ifremer/CNRS/IRD/Editions scientifiques et medicales Elsevier SAS. All rights reserved.
Tipo: Text
Palavras-chave: Cartographie; Phanérogames marines; Posidonia oceanica; Méditerranée; Mapping; Seagass; Posidonia oceanica; Mediterranean Sea.
Ano: 2002
URL: http://archimer.ifremer.fr/doc/00322/43314/42940.pdf