Consulta: subjectFacets:"Soil resistance"
Registros recuperados: 5
Data/hora: 05/06/2024 11:36:14

Avaliação de qualidade do solo no sistema ILPF (URTP Embrapa Milho e Sorgo).
Provedor de dados: Informação Tecnológica em Agricultura (Infoteca-e)
Autores: ALBUQUERQUE FILHO, M. R. de; VIANA, J. H. M.; CLEMENTE, E. de P.
RESUMO - Os níveis de resistência à penetração do solo e a qualidade da estrutura na camada superficial foram avaliados na Unidade de Referência em sistema ILPF e no cerrado adjacente, na Fazenda Experimental da Embrapa Milho e Sorgo, em Sete Lagoas-MG. O trabalho foi realizado utilizando-se um penetrógrafo eletrônico para avaliar a resistência do solo à penetração até 60 cm de profundidade e o DRES - Diagnóstico Rápido da Estrutura do Solo para a camada de 0 a 20 cm de profundidade. Não houve diferença estatística entre a resistência à penetração no cerrado e no sistema ILPF. A camada de maior resistência no ILPF se localiza mais próxima à superfície e com densidade um pouco mais elevada, mas abaixo do limite de impedimento ao crescimento de raízes e...
Tipo: Folhetos
Palavras-chave: Resistência do solo; Penetração; DRES; Penetrometria; Soil resistance; Penetrometry; Manejo do Solo; Sistema de Cultivo.
Ano: 2022
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1149570

Measuring mechanical impedance in clayey gravelly soils
Provedor de dados: Revista Brasileira de Ciência do Solo
Autores: Stolf,R.; Cassel,D. K.; King,L. D.; Reichardt,K.
Mechanical impedance of clayey and gravelly soils is often needed to interpret experimental results from tillage and other field experiments. Its measurement is difficult with manual and hydraulic penetrometers, which often bend or break in such soils. The purpose of this study was to evaluate the feasibility of a hand-operated "Stolf" impact penetrometer to measure mechanical impedance (soil resistance). The research was conducted in Raleigh, North Carolina, USA (35º 45'N, 78º 42'W, elevation 75 m). Corn was planted on April 19, 1991. Penetrometer measurements were taken on May 10, 1991, in 5 cm intervals to 60 cm at 33 locations on a transect perpendicular to the corn rows in each of four tillage treatments. The data permitted three-dimensional displays...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Impact penetrometer; Soil resistance; Hard clayey and gravelly soils; Spatial distribution.
Ano: 1998
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06831998000200003

Estimating Sample Size of Soil Cone Index Profiles by Bootstrapping
Provedor de dados: Revista Brasileira de Ciência do Solo
Autores: Alesso,Carlos Agustín; Masola,María Josefina; Carrizo,María Eugenia; Imhoff,Silvia Del Carmen.
ABSTRACT Measurements of the soil cone index are widely used to assess soil resistance to root penetration (SR) and to monitor the soil compaction status of agricultural fields. However, soil sampling for SR estimation is a rather challenging task in view of the high spatial and temporal variability of the soil. This study proposed a bootstrapping method to determine the minimum sample size required to estimate the vertical profile of mean soil cone index (CI) values at different levels of precision and confidence. For this purpose, CI data from a Typic Argiudoll under no-tillage before and after chiseling was used. A total of 151 CI profiles were recorded before and after chiseling in a 3,200 m2 (40 × 80 m) no-tillage area at sampling points distributed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sampling; Soil resistance; Bootstrap procedure; Soil variability.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832017000100429

Aggregate stability and penetration resistance after mobilization of a dystrocohesive Ultisol
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Tavares,Uilka E.; Rolim,Mario M.; Simões Neto,Djalma E.; Pedrosa,Elvira M. R.; Magalhães,Adriana G.; Silva,Ênio F. de F. e.
ABSTRACT Evaluation of mobilized soil profiles can provide important information on soil compaction reduction processes. In this context, the objective of this study was to evaluate alterations in soil penetration resistance and the impact on the aggregate stability of a cohesive Ultisol cultivated with sugarcane. The experiment was carried out at the Carpina Sugarcane Experimental Station (EECAC/UFRPE), located in the city of Carpina, PE. Penetration resistance, mobilized area and depth, and percentage of soil aggregates were evaluated before and after soil tillage. Soil mobilization improved soil aggregate uniformity and decreased penetration resistance in the 0-0.20 m layer. Coarse soil fraction, moisture and organic carbon positively contributed to the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Furrowing; Harrowing; Soil resistance.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017001100752

Mapping soil compaction using indicator kriging in Santa Fe province, Argentina
Provedor de dados: Acta Agronómica
Autores: Agustín-Alesso,Carlos; Carrizo,María Eugenia; del-Carmen-Imhoff,Silvia.
Abstract Soil compaction is a complex physical process that affects the crop performance by limiting the expansion of the roots and the reduction of water and nutrients uptake from soil. Due to the spatial variability of soil compaction, the needs for remedial practices may vary within the field. However, mapping soil compaction estimated by cone index (CI) data is a difficult task. The aim of this study were to examine the spatial variability of CI data in a fine-mixed-thermic Typic Argiudoll soil form the center of Santa Fe, province -Argentina under no-till system, and to delineate zones for site-specific tillage based on maps of probabilities of occurrence of soil compaction developed using indicator kriging. Sixty nine georeferenced CI and volumetric...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cone index; Potential site-specific tillage management zones; Soil resistance; Spatial variability; Variography.
Ano: 2017
URL: http://www.scielo.org.co/scielo.php?script=sci_arttext&pid=S0120-28122017000100081