Consulta: subjectFacets:"Soil salinization"
Registros recuperados: 4
Data/hora: 04/06/2024 10:07:07

Assessment of opportunities to map pearl millet tolerance to salinity during germination and early seedling growth
Provedor de dados: 30
Autores: Mukhopadhyay, R.
Palavras-chave: Millets; Tolerance; Genotypes; Phenotypes; Genetic markers; Genomes; Heritability; Soil salinization; Feed crops; Humus.
Ano: 2005
URL: http://agropedia.iitk.ac.in/openaccess/?q=node/3215

Response of Selected Sorghum Lines to Soil Salinity-Stress under Field Conditions
Provedor de dados: 30
Autores: Ramesh, S.
Palavras-chave: Soil salinization; Sorghum; Hybrids; Heritability; Phenotypes; Genotypes; Grain; Statistical methods; Genetic improvement; Tolerance.
Ano: 2005
URL: http://agropedia.iitk.ac.in/openaccess/?q=node/3261

A proposed index to assess quality of waters from desalination plants
Provedor de dados: 91
Autores: Antas,Francisco P. de S.; Freitas,Jair J. R. de; Oliveira,André M. de; Dias,Nildo da S.; Lima,Alexandre de O.; Sousa Neto,Osvaldo N. de.
ABSTRACT Reverse osmosis is the technology commonly used to produce fresh water from brackish groundwater. Due to the reject brine generated in desalination plants by reverse osmosis, vulnerability assessment to define critical areas to monitor waters from desalination has been an important tool for delineating the monitoring networks required for surveillance of potential salinization sites. The objective of this study was to assess the quality of waters sampled in desalination plants by a quality index, which provides a relative assessment of water vulnerability to potential salinization. The present study proposes an index to assess the quality of waters from desalination plants initially using the chemical parameters electrical conductivity, sodium...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil salinization; Brackish well water; Groundwater contamination.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662018001000667

Physicochemical changes of semiarid soil submitted to treated wastewater, with and without cultivar
Provedor de dados: 109
Autores: Conceição-Silva,Solange; Oliveira,Iara Brandão de; Pinto-Medeiros,Yvonilde Dantas; Silva-Paz,Vital Pedro da.
Abstract This work evaluated the changes in physicochemical attributes in semiarid soil submitted to domestic sewage submitted to anaerobic treatment, in the presence or absence of the cultivar. The experimental unit was set up in the rural area of Ouro Verde, municipality of São Domingos, state of Bahia, Brazil. Five treatments were tested by diluting wastewater and supply in the percentages 0 %, 25 %, 50 %, 75 %, and 100 %. Soil samples were taken at depths of 0 - 35 cm (P1), and 35 - 70 cm (P2) from the sampling units with cultivar, control units without cultivar, and the unit without treatment (white). The cultivar was of corn (Zea mays L.), of the family Poaceae, which has a relatively short cycle (60 - 120 days). At the end of the experiments, after...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Treated domestic wastewater; Anaerobic process; Semi-arid region; Soil salinization; Soil sodification.
Ano: 2022
URL: http://www.scielo.org.co/scielo.php?script=sci_arttext&pid=S0120-28122022000300258