Consulta: subjectFacets:"Sulphate reduction"
Registros recuperados: 2
Data/hora: 09/06/2024 05:30:23

Effect of sulphate concentration and sulphide desorption on the combined removal of organic matter and sulphate from wastewaters using expanded granular sludge bed (EGSB) reactors
Provedor de dados: 69
Autores: Valdés,Freddy; Muñoz,Edmundo; Chamy,Rolando; Ruiz,Gonzalo; Vergara,Christian; Jeison,David.
During the application of anaerobic processes to high sulphate concentration wastewaters, operational problems are expected due to the occurrence of sulphate reduction. Sulphide production reduces effluent quality and may produce inhibition. The application of Expanded Granular Sludge Bed (EGSB) reactors for the combined removal of organic matter and sulphate was studied at different COD/sulphate and 3 values of pH. During the EGSB reactor operation, most of the sulphide remains in the liquid phase reducing effluent quality. The inclusion of a desorption column in the recirculation of the EGSB reactor promotes mass transfer to the gas phase, reducing the sulphide concentration in the liquid phase, significantly decreasing the chemical oxygen demand of the...
Tipo: Journal article
Palavras-chave: Anaerobic digestion; EGSB; Sulphate reduction; Sulphide.
Ano: 2006
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0717-34582006000400004

Complex coupled metabolic and prokaryotic community responses to increasing temperatures in anaerobic marine sediments: critical temperatures and substrate changes
Provedor de dados: 5
Autores: Roussel, Erwan; Cragg, Barry A.; Webster, Gordon; Sass, Henrik; Tang, Xiaohong; Williams, Angharad S.; Gorra, Roberta; Weightman, Andrew J.; Parkes, R. John.
The impact of temperature (0 - 80°C) on anaerobic biogeochemical processes and prokaryotic communities in marine sediments (tidal flat) was investigated in slurries for up to 100 days. Temperature had a non-linear effect on biogeochemistry and prokaryotes with rapid changes over small temperature intervals. Some activities (e.g. methanogenesis) had multiple “windows” within a large temperature range (~10 - 80°C). Others, including acetate oxidation, had maximum activities within a temperature zone, which varied with electron acceptor (metal oxide [up to ~34°C] and sulphate [up to ~50°C]). Substrates for sulphate reduction changed from predominantly acetate below, and H2 above, a 43°C critical temperature; along with changes in activation energies and types...
Tipo: Text
Palavras-chave: Sediment; Temperature; Anaerobic processes; Chemoorganotrophic; Chemolithotrophic; Mineralisation; Sulphate reduction; Methanogenesis; Acetogenesis.
Ano: 2015
URL: https://archimer.ifremer.fr/doc/00273/38464/36883.pdf