Data/hora: 27/07/2024 03:17:00

Provedor de dados: 	5	
País: 	France	
Título: 	Delayed mode quality control and Oxygen correction of Ovide Argo data. Float WMO 1901206	
Autores: 	Lagadec, Catherine; Thierry, Virginie; Cabanes, Cecile.	
Data: 	2017-11-08	
Ano: 	2017	
Resumo: 	This report presents the delayed mode analysis of an Argo float. Real time quality control are checked and interesting profiles are plotted. The OW method (objective analysis) is used to detect a conductivity sensor drift and correct it, if any. In this report, are also explained and plotted Oxygen corrections with LOCODOX software.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00409/52036/52702.pdf

http://archimer.ifremer.fr/doc/00409/52036/	
Formato: 	application/pdf	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use