Consulta: creatorFacets:"Neichel, B."
Registros recuperados: 1
Data/hora: 27/07/2024 01:54:49

Pyramid wavefront sensor optical gains compensation using a convolutional model
Provedor de dados: 5
Autores: Chambouleyron, V; Fauvarque, Olivier; Janin-potiron, P.; Correia, C.; Sauvage, J-f; Schwartz, N.; Neichel, B.; Fusco, T.
Context. Extremely large telescopes are overwhelmingly equipped with pyramid wavefront sensors (PyWFS) over the more widely used Shack-Hartmann wavefront sensor to perform their single-conjugate adaptive optics (SCAO) mode. The PyWFS, a sensor based on Fourier filtering, has proven to be highly successful in many astronomy applications. However, this sensor exhibits non-linear behaviours that lead to a reduction of the sensitivity of the instrument when working with non-zero residual wavefronts. This so-called optical gains (OG) effect, degrades the closed-loop performance of SCAO systems and prevents accurate correction of non-common path aberrations (NCPA).Aims. In this paper, we aim to compute the OG using a fast and agile strategy to control PyWFS...
Tipo: Text
Palavras-chave: Instrumentation: adaptive optics; Atmospheric effects.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00666/77856/80014.pdf