Consulta: creatorFacets:"Rocha Junior,Romero C."
Registros recuperados: 2
Data/hora: 27/07/2024 02:54:28

DELIMITATION OF HOMOGENEOUS ZONES IN VINEYARDS USING GEOSTATISTICS AND MULTIVARIATE ANALYSIS OF DIFFERENT VEGETATION INDICES
Provedor de dados: Engenharia Agrícola
Autores: Costa,Bruno R. S.; Oldoni,Henrique; Rocha Junior,Romero C.; Bassoi,Luís H.
ABSTRACT Vegetation indices (VIs) are quantitative measures used to describe the distribution and spatial variability of the vegetation cover of natural or cultivated areas. The aim of this study was to delimit homogeneous zones (HZs) of different VIs using geostatistics and multivariate analysis in order to identify vegetation patterns in Cabernet Franc and Cabernet Sauvignon vineyards. The evaluation was performed in two vineyards in the municipality of Espírito Santo do Pinhal in the state of São Paulo, Brazil. Reflectance (ρ) was measured at three wavelengths of the electromagnetic spectrum (670, 730, and 780 nm) at canopy height in georeferenced points along planting rows using the Crop Circle ACS-430 active sensor. Nine VIs were calculated based on...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vitis vinifera L.; Canopy density; Agricultural instrumentation.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800013

EFFECTS OF SIZE AND SAMPLING GRID ON THE QUALITY OF APPARENT SOIL ELECTRICAL CONDUCTIVITY MAPS
Provedor de dados: Engenharia Agrícola
Autores: Oldoni,Henrique; Costa,Bruno R. S.; Rocha Junior,Romero C.; Rabello,Ladislau M.; Bassoi,Luís H.
ABSTRACT The apparent soil electrical conductivity (ECa) is an attribute commonly used for the characterization of the spatial variability of soil, but its determination by handheld sensors consumes considerable time and labor. The reduction in the number of sampling points allows minimize them but can result in increased uncertainty of interpolated maps. Thus, the goal of this study was to identify the best spacing and number of ECa measurements, to guarantee the quality of maps generated in three vineyards. The ECa values were obtained using a handheld sensor in different sampling grids. The data were submitted to descriptive statistical and geostatistical analyses. The relative deviation and Kappa coefficient of agreement were used to assess the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spatial variability; Geostatistics; Agricultural instrumentation.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800001