Consulta: creatorFacets:"Serra, Romain"
Registros recuperados: 2
Data/hora: 27/07/2024 08:14:42

Processing Bio-Argo nitrate concentration at the DAC Level
Provedor de dados: 5
Autores: Johnson, Ken; Pasqueron De Fommervault, Orens; Serra, Romain; D'Ortenzio, Fabrizio; Schmechtig, Catherine; Claustre, Hervé; Poteau, Antoine.
The only method used to date to measure dissolved nitrate concentration (NITRATE) with sensors mounted on profiling floats is based on the absorption of light at ultraviolet wavelengths by nitrate ion (Johnson and Coletti, 2002; Johnson et al., 2010; 2013; D’Ortenzio et al., 2012). Nitrate has a modest UV absorption band with a peak near 210 nm, which overlaps with the stronger absorption band of bromide, which has a peak near 200 nm. In addition, there is a much weaker absorption due to dissolved organic matter and light scattering by particles (Ogura and Hanya, 1966). The UV spectrum thus consists of three components, bromide, nitrate and a background due to organics and particles. The background also includes thermal effects on the instrument and slow...
Tipo: Text
Ano: 2018
URL: http://archimer.ifremer.fr/doc/00350/46121/55922.pdf

Two databases derived from BGC-Argo float measurements for marine biogeochemical and bio-optical applications
Provedor de dados: 5
Autores: Organelli, Emanuele; Barbieux, Marie; Claustre, Herve; Schmechtig, Catherine; Poteau, Antoine; Bricaud, Annick; Boss, Emmanuel; Briggs, Nathan; Dall'Olmo, Giorgio; D'Ortenzio, Fabrizio; Leymarie, Edouard; Mangin, Antoine; Obolensky, Grigor; Penkerc'H, Christophe; Prieur, Louis; Roesler, Collin; Serra, Romain; Uitz, Julia; Xing, Xiaogang.
Since 2012, an array of 105 Biogeochemical-Argo (BGC-Argo) floats has been deployed across the world's oceans to assist in filling observational gaps that are required for characterizing open-ocean environments. Profiles of biogeochemical (chlorophyll and dissolved organic matter) and optical (single-wavelength particulate optical backscattering, downward irradiance at three wavelengths, and photosynthetically available radiation) variables are collected in the upper 1000 m every 1 to 10 days. The database of 9837 vertical profiles collected up to January 2016 is presented and its spatial and temporal coverage is discussed. Each variable is quality controlled with specifically developed procedures and its time series is quality-assessed to identify issues...
Tipo: Text
Ano: 2017
URL: https://archimer.ifremer.fr/doc/00662/77389/79010.pdf