Data/hora: 27/07/2024 02:00:09

Provedor de dados: 	21	
País: 	Germany	
Título: 	Energy efficiency of fossil and renewable fuels	
Autores: 	Schäfer, Winfried.	
Data: 	2016-01-13	
Ano: 	2016	
Palavras-chave: 	Air and water emissions.	
Resumo: 	Assessment results of renewable energy supply in agriculture and forestry are often questionable because 1. the methodology does not describe the nature dependent conditions of agricultural production, 2. there is no standard system boundary, 3. thermodynamic laws are violated and/or ignored, 4. direct and embodied energy is mixed, 5. the mainstream life cycle analysis (LCA) takes downstream and upstream inputs arbitrarily  into  consideration,  depending  on  the  research  objectives  and  the  research-funding  agency. Thus, the calculation results neglect a wide range of specific energy input figures of upstream and downstream factors outside farm level resulting in non-comparable figures.    The EROI describes the ratio between energy output and input. The advantage of this measure is that energy input and output of fuel supply as well as the resulting CO2 emissions are comparable. There are no standards to calculate the indirect energy input of commodities and services hidden in monetary inputs (insurances, rent for land, subsidies and fees etc.). They are usually excluded because procedures to handle them as energy input are rare. The easiest way to quantify the indirect energy is the use of the energy  intensity  (EI).  Multiplying  the  price  of  any  good  or  service  with  the  energy  intensity  results  in  a rough estimation of energy embodied in the good or service. Applying the EROI and the EI to compare   the efficiency of fossil and renewable energy supply released the following results:     Substitution of fossil fuels by renewable ones causes always additional costs. Most known renewable energy supply techniques need more energy than fossil fuel exploitation. Polluting the environment is - for the time being – the most competitive alternative. Renewable engine fuel, produced from biomass, is not competitive with fossil fuels in terms of EROI. The energy of one ha biomass may substitute gasoline to drive a car 40 000 km with biogas. Electric power harnessed from one ha solar panels enables to drive   an electric vehicle 5 000 000 km applying the same calculation method. The most efficient way to mitigate CO2 emissions is to include the entropy of agricultural products in energy policy decision making. Albeit wood has a high EROI, processing fuels from wood of low entropy makes no sense: Producing a table from a tree and burning the residues and the table at the end of its lifetime renders the same energy gain as using the tree for fuel only. The EROI of fossil fuels remains probably on high level during the next 50 to 100 years. Oil and gas will be replaced by coal, in Finland also by nuclear power, peat and wood. Although biomass is more renewable than fossil fuels, its EROI is lower and substitution will not reduce CO2 emissions.     Climate change may force humankind to reduce fossil fuel consumption. The only sustainable way   to achieve this is reduction of fossil fuel exploitation	
Tipo: 	Conference paper, poster, etc.	
Identificador: 	Schäfer, Winfried    (2016) Energy efficiency of fossil and renewable fuels.       Paper at:   Maataloustieteen päivät 2016, , Viikki, Helsinki, 12.–13.1.2016.	
Editor: 	Suomen Maataloustieteellisen Seuran	
Relação: 	http://orgprints.org/29742/