Consulta: subjectFacets:"Bio-argo"
Registros recuperados: 3
Data/hora: 27/07/2024 03:09:21

Processing Argo oxygen data at the DAC level
Provedor de dados: 5
Autores: Thierry, Virginie; Bittig, Henry; Gilbert, Denis; Kobayashi, Taiyo; Kanako, Sato; Schmid, Claudia.
This document does NOT address the issue of oxygen data quality control (either real-time or delayed mode). As a preliminary step towards that goal, this document seeks to ensure that all countries deploying floats equipped with oxygen sensors document the data and metadata related to these floats properly. We produced this document in response to action item 14 from the AST-10 meeting in Hangzhou (March 22-23, 2009). Action item 14: Denis Gilbert to work with Taiyo Kobayashi and Virginie Thierry to ensure DACs are processing oxygen data according to recommendations. If the recommendations contained herein are followed, we will end up with a more uniform set of oxygen data within the Argo data system, allowing users to begin analysing not only their own...
Tipo: Text
Palavras-chave: Argo; Bio-argo; Oxygen.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00287/39795/59750.pdf

SCOR WG 142: Quality Control Procedures for Oxygen and Other Biogeochemical Sensors on Floats and Gliders. Recommendation for oxygen measurements from Argo floats, implementation of in-air-measurement routine to assure highest long-term accuracy
Provedor de dados: 5
Autores: Bittig, Henry; Kortzinger, Arne; Johnson, Ken; Claustre, Hervé; Emerson, Steve; Fennel, Katja; Garcia, Hernan; Gilbert, Denis; Gruber, Nicolas; Kang, Dong-jin; Naqvi, Wajih; Prakash, Satya; Riser, Steven; Thierry, Virginie; Tilbrook, Bronte; Uchida, Hiroshi; Ulloa, Osvaldo; Xing, Xiagang.
Recommendation for Oxygen Measurements from Argo Floats: Implementation of In-Air-Measurement Routine to Assure Highest Long-term Accuracy  As Argo has entered its second decade and chemical/biological sensor technology is improving constantly, the marine biogeochemistry community is starting to embrace the successful Argo float program. An augmentation of the global float observatory, however, has to follow rather stringent constraints regarding sensor characteristics as well as data processing and quality control routines. Owing to the fairly advanced state of oxygen sensor technology and the high scientific value of oceanic oxygen measurements (Gruber et al., 2010), an expansion of the Argo core mission to routine oxygen measurements is perhaps the most...
Tipo: Text
Palavras-chave: Argo; Bio-argo; Oxygen.
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00348/45917/46180.pdf

SCOR WG 142: Quality Control Procedures for Oxygen and Other Biogeochemical Sensors on Floats and Gliders. Recommendations on the conversion between oxygen quantities for Bio-Argo floats and other autonomous sensor platforms
Provedor de dados: 5
Autores: Bittig, Henry; Körtzinger, Arne; Johnson, Ken; Claustre, Herve; Emerson, Steve; Fennel, Katja; Garcia, Hernan; Gilbert, Denis; Gruber, Nicolas; Kang, Dong-jin; Naqvi, Wajih; Prakash, Satya; Riser, Steven; Thierry, Virginie; Tilbrook, Bronte; Uchida, Hiroshi; Ulloa, Osvaldo; Xing, Xiaogang.
Tipo: Text
Palavras-chave: Argo; Bio-argo; Oxygen.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00348/45915/56281.pdf