Data/hora: 27/07/2024 02:14:49

Provedor de dados: 	Brazilian Archives of Biology and Technology	
País: 	Brazil	
Título: 	Start-up and steady-state conditions of an Anaerobic Hybrid Reactor (AHR) using mini-filters composed with two types of support medium operating under low loading rates	
Autores: 	Silva,Vivian Galdino da; Campos,Cláudio Milton Montenegro; Pereira,Erlon Lopes; Silva,Júlia Ferreira da.	
Data: 	2011-10-01	
Ano: 	2011	
Palavras-chave: 	Environmental chemistry; Coffee wastewater; Biodegradation; Optimization process.	
Resumo: 	The present work aimed at studying the operational parameters of an Anaerobic Hybrid Reactor (AHR) removing organic matter of coffee wastewater with low concentration. The AHR was built similar to an UASB reactor, however the interior was filled with mini-filters composed by two types of support materials: expanded clay and rolled pebble. Three start-ups were accomplished in order to achieve the stationary state (steady-state). Three hydraulic retention times were appraised: 28.5; 24.0 and 18.0 h, obtaining a volumetric loading rate (VLR) of 0.70; 0.56; 0.54 kg COD m-3 d-1 and a biological organic loading rate (BOLR) of 0.0156; 0.0103 and 0.01213 kg BOD5 kg TVS-1 d-1. Due to the decrease in the concentration of organic matter in the influent, the endogen process started to occur on the biomass lowering the methanogenic process.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132011000500015	
Editor: 	Instituto de Tecnologia do Paraná - Tecpar	
Relação: 	10.1590/S1516-89132011000500015	
Formato: 	text/html	
Fonte: 	Brazilian Archives of Biology and Technology  v.54 n.5 2011	
Fonte: 	info:eu-repo/semantics/openAccess