Data/hora: 01/06/2024 16:32:47

Provedor de dados: 	107	
País: 	Brazil	
Título: 	GAINS IN PERFORMANCE OF DIESEL CYCLE ENGINE USING B10

GAINS IN PERFORMANCE OF DIESEL CYCLE ENGINE USING B10 COMPARED TO OTHER MIXTURES	
Autores: 	Guimarães, Camila Coelho; Santos, Vivianni Marques Leite dos; Dantas, Alan Christie da Silva; Cortez, Jorge Wilson; Pereira, Paulo José.	
Data: 	2018-04-20	
Ano: 	2018	
Palavras-chave: 	Energia na Agricultura consumption; Dynamometer test; Power; Torque.	
Resumo: 	Studies to develop renewable fuels, such as biodiesel, as substitutes for petroleum diesel are of great environmental importance. However, to be effectively incorporated into the energy mix, satisfactory performance of a diesel cycle engine under the effect of this biofuel must be ensured. The objective of this study was to evaluate the specific fuel consumption, effective power and torque of a diesel engine with respect to resistive loads under varying volumetric proportions of soybean biodiesel in diesel mineral oil (5% (B5), 10% (B10), 25% (B25) and 50% (B50)) under varying applied loads (1.5, 3.0, 4.5, 6.0, 7.5 and 9.0 kW). For the test, a 7.36 kW engine coupled to a 28.8 kW three-phase electric generator was used. The loads were elevated up to 9.0 kW via a three-phase resistive bench. In terms of power and torque, the performances of the B5 and B10 mixtures were not significantly different, whereas the B25 and B50 mixtures displayed lower performances. The B10 mixture showed better performance in terms of consumption because the remaining mixtures had results similar to those of the B5 mixture.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Português	
Identificador: 	http://www.seer.ufv.br/seer/index.php/reveng/article/view/762

10.13083/reveng.v26i2.762	
Editor: 	Universidade Federal de Viçosa - UFV	
Relação: 	http://www.seer.ufv.br/seer/index.php/reveng/article/view/762/pdf	
Formato: 	application/pdf	
Fonte: 	REVISTA ENGENHARIA NA AGRICULTURA - REVENG; v. 26, n. 2 (2018): MARÇO/ABRIL; 124-132

2175-6813

1414-3984