Data/hora: 02/06/2024 18:23:15

Provedor de dados: | 111
País: | China
Título: | Effect of Some Threshing Parameters on Sesame Separation
Autores: | D. Yilma; Akdeniz University,; I. Akinci; M. I. Cagirgan.
Data: | 1969-12-31
Ano: | 1969
Resumo: | The threshing section on combine harvester or thresher machine affects grain and stalk separation performance. In this study, effect of some threshing parameters such as drum speed, feed rate and concave open on closed capsules sesame straw sieve in developed threshing unit. Threshing drums used were a rasp bar with tooth type. Three threshing drum speeds of 500, 700 and 900 min-1 (6.5, 9.1, 11.7 m/s) were used to investigations. Three feed rate as 90, 180 and 270 kg/h and three concave open as 20, 35 and 50 mm were used in this study. Four sieves were used for separation of straw. Their mesh numbers are 7, 10, 14 and 18. Results show that the best performance for separation of sesame straw were gave at the maximum drum speeds, minimum feed rates and concave opens experienced in this study.
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/1236
Editor: | International Commission of Agricultural and Biosystems Engineering
Formato: | application/pdf
Fonte: | Agricultural Engineering International: CIGR Journal; Volume X (2008)
Fonte: | &lt;html /&gt;