Data/hora: 11/06/2024 15:00:18

Provedor de dados: | 111
País: | China
Título: | Anthropometric studies for designing to fit gari-frying workers
Autores: | aremu, olaniyi olateju; salami, ismaila olasunkanmi; Adetifa, Babatunde o; Onu, Livinus i; Adegbite, adeyemi E; olokoshe, abimbola a; Samuel, Taiwo Moses.
Data: | 2016-03-22
Ano: | 2016
Palavras-chave: | Ergonomics; Anthropometry anthropometry  workstation  gari-frying  cassava processing  design to fit  BMI  BSA.
Resumo: | Work system and product design require anthropometric data of the user population relevant to the facility in order to have safe operation in service as well as increase user satisfaction and efficiency. Designing to fit gari-frying workers in each of the southwestern states in Nigeria is geared towards this end. The age, weight and twenty-five body dimensions of 120 gari-frying workers in Lagos, Ogun, Oyo, Osun, Ondo and Ekiti, selected by random sampling, were measured. The body dimensions include stature, shoulder height, sitting height, eye height, forward grip reach, buttock-popliteal height, buttock-knee length, knee height, thigh clearance, forearm-to-forearm breadth, waist depth, elbow rest height, knuckle height, elbow grip length, hip breadth, hand length, hand breadth, hand thickness, grip span and lumbar height. SPSS 20 software was used to perform statistical analysis to determine the mean, standard deviation, minimum and maximum values, 2nd, 5th, 25th, 50th, 75th and 95th percentiles for each state. Ogun state was used as a control, against which means of body dimension data, collected from other states, were compared using paired sample t-test. The results revealed that some of the body dimensions showed significant difference across the states at P≤0.05 with Oyo having more anthropometric parameters that differ from that of Ogun and Ondo having the least. Between 11.42% and 24.25% difference in the mean age, weight and lumbar height was observed in all the states. Osun state has the highest mean BMI and BSA values of 32.38 kg/m2 and 1.82 m2, respectively. These results are the required data for the design of facility and products for gari-frying workers as well as in similar women workspaces, especially in processing centres.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/3403
Editor: | International Commission of Agricultural and Biosystems Engineering
Relação: | http://www.cigrjournal.org/index.php/Ejounral/article/view/3403/2294
Formato: | application/pdf

Fonte:

Agricultural Engineering International: CIGR Journal; Vol 18, No 1 (2016): CIGR Journal; 180-191

1682-1130

Fonte: | Copyright (c) 2016 Agricultural Engineering International: CIGR Journal