Data/hora: 12/06/2024 04:27:35

Provedor de dados: 	111	
País: 	China	
Título: 	Effect of Conservative Tillage on Physical Properties of Soil and Yield of Rainfed Wheat	
Autores: 	Younesi Alamooti, Mohammad.	
Data: 	2020-03-15	
Ano: 	2020	
Palavras-chave: 	Agricultural Machinery Department; Agricultural Engineering Research Institute Rainfed agriculture; Conservative tillage; Energy consumption; Wheat.	
Resumo: 	     In order to study the effect of conservative tillage on a number of physical properties of soil and the yield of rainfed wheat, an experiment in form of a randomized complete block design (RCBD) with three replications was conducted in a field in Aliabad County, Iran. The study treatments included: T1) Conventional method, T2) Combined moldboard plow method, T3) Chisel-packer method, and T4) Direct planting method. During early October, the study soil was prepared based on these treatments in a field which was used for rainfed wheat farming in the the previous year. The apparent specific gravity of soil, weighted mean diameter (WMD) of soil aggregates, soil mechanical resistance, and soil permeability were measured. Data were analyzed in MSTAT-C. Results showed that the tillage practice had no significant effect on grain yield (p &lt; 0.05). Soil permeability was 10.9, 16.3, 15.7 and 17.9 mm/h for T1, T2, T3 and T4, respectively.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/5111	
Editor: 	International Commission of Agricultural and Biosystems Engineering	
Relação: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/5111/3237

http://www.cigrjournal.org/index.php/Ejounral/article/downloadSuppFile/5111/2345	
Formato: 	application/pdf	
Fonte: 	Agricultural Engineering International: CIGR Journal; Vol 22, No 1 (2020): CIGR Journal; 48-53

1682-1130	
Fonte: 	Copyright (c) 2020 Agricultural Engineering International: CIGR Journal