Data/hora: 12/06/2024 14:43:48

Provedor de dados: | 111
País: | China
Título: | Quasi-static and impact cutting behavior definition of privet stem
Autores: | Kamandar, Mohammad Reza; Massah, Jafar; Khanali, Majid.
Data: | 2018-06-18
Ano: | 2018
Palavras-chave: | Quasi-static cutting; Impact cutting; Shear energy; Shear strength; Privet.
Resumo: | Some of agricultural operations such as privet stem pruning are slowly, repetitive and occasionally dangerous for operators. Almost operators of privet trimmers are exposed to the unpleasant and dangerous arm and body vibrations and sound of pruning machines. The knowing of the shearing behaviors of privet stem have important role in the design and fabricate of suitable pruning machine. So a series of experimental tests were performed to measuring the shear force, shear consumption energy and shear strength of stem internodes of privet stalk under quasi-static and impact cutting at different loading rate, different internode position and moisture level 58% wet base. In the quasi-static cutting test, the stalk specimens were cut in the quasi-static process at four loading rates: 5, 10, 15 and 20 mm/min and three internode positions: fifth, tenth and fifteenth. In impact cutting test, the stalk specimens were served in impact process at four loading rates: 1, 2, 3 and 4 m/s and three internode positions: fifth, tenth and fifteenth. In quasi-static cutting, the variance analysis of the data indicated that the loading rate, created significant effect on shear strength and shear consumption energy in probability level of 5%. Also the internode position and the interaction effect of loading rate and internode position, created significant effects on shear strength and shear consumption energy in probability level of 1%. Based on the statistical analysis, the average values of shear consumption energy and shear strength were obtained as 556.70 J from 95.35 to 1567.95 J and 29.12 Mpa from 19.63 to 37.04 Mpa respectively. In impact cutting, the variance analysis of the data results showed that the effect of loading rate, the effect of internode position and interaction effect of loading rate on internode position, created significant effect on shear consumption energy and shear strength in probability level of 1%. The data statistical analysis showed the average values of shear consumption energy and shear strength were obtained as 17.16 J from 3.19 to 28.60 J and 1.01 Mpa from 0.21 to 2.53 Mpa respectively.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/4282
Editor: | International Commission of Agricultural and Biosystems Engineering

Relação:

http://www.cigrjournal.org/index.php/Ejounral/article/view/4282/2694

http://www.cigrjournal.org/index.php/Ejounral/article/downloadSuppFile/4282/1712

http://www.cigrjournal.org/index.php/Ejounral/article/downloadSuppFile/4282/1713

Formato: | application/pdf

Fonte:

Agricultural Engineering International: CIGR Journal; Vol 20, No 1 (2018): CIGR Journal; 70-80

1682-1130

Fonte: | Copyright (c) 2018 Agricultural Engineering International: CIGR Journal