Data/hora: 17/06/2024 03:50:58

Provedor de dados: | 111
País: | China
Título: | Noise evaluation of MF285 tractor while pulling a trailer in an asphalt road
Autores: | Farzad Jalilian tabar; Hekmat Rabbani; Agricultural Machinery Department, Razi University of Kermanshah, Iran; Alinejat Lorestani; Agricultural Machinery Department, Razi University of Kermanshah, Iran; Payam Javadikia; Agricultural Machinery Department, Razi University of Kermanshah, Iran; Rashid Gholami; Agricultural Machinery Department, Razi University of Kermanshah, Iran;.
Data: | 2012-12-24
Ano: | 2012
Palavras-chave: | Noise; Tractor; Sound pressure level; Ergonomics.
Resumo: | Tractors have been used for transportation on roads by many farmers in addition to use in the field operations. MF285 tractor is the popular kind of tractor in Iran (about 30% of all tractors) and almost this tractor has been used without cabin.  Despite the problems caused by noise from the tractors and all its adverse effects on users and observers, no comprehensive research has been done on them.  The result of this research indicate that the noise level of MF285 tractor, in 2250 r/min engine speed, will be 90 dB(A) which in comparison with the standard value, 85 dB(A), is dangerous for operator’s ears.  The test site was prepared according to the international standards.  The noise emitted by tractor in three gears (2, 3 and 4) and three speeds (1,500, 1,950 and 2,250 r/min) were measured and then analyzed statistically.  Analysis of variance and Duncan’s mean comparison test showed that the Sound Pressure Level (SPL) at the position of the driver in comparison to the observer position was statistically significant (P
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/2096
Editor: | International Commission of Agricultural and Biosystems Engineering
Relação: | http://www.cigrjournal.org/index.php/Ejounral/article/download/2096/5339
Formato: | application/pdf
Fonte: | Agricultural Engineering International: CIGR Journal; Vol 14, No 4 (2012): CIGR Journal; 50-55
Fonte: | &lt;html /&gt;