Data/hora: 01/06/2024 16:45:55

Provedor de dados: | 111
País: | China
Título: | Application of Urine as Fuel in a Soil-based Membrane-less Single Chamber Microbial Fuel Cell
Autores: | Simeon, Meshack Imologie; Otache., Matins Yusuf; Ewemojie, Temitayo Abayomi; RAJI, AbdulGaniy Olayinka.
Data: | 2019-04-30
Ano: | 2019
Palavras-chave: | Renewable Energy; Microbial Fuel Cell Technology Soil; Urine; Microorganism; Power; Fuel Cell.
Resumo: | Microbial fuel cell (MFC) technology is a promising bio-technology that utilizes the microorganism in organic wastes to generate electricity. Although human urine has been identified as a suitable substrate in MFCs, its possible utilization in a soil-based Membrane-less Single Chamber Microbial Fuel Cell (MSCMFC) for constant power generation has, hitherto, not been reported. In this study, a MFC was set up with mud as inoculums in a plastic cylindrical vessel using carbon felt electrodes. It was operated for 19 days (456 hours) without extra substrate. Then, the MFC was treated with human urine (as substrate) four times (Days 19, 24, 32 and 36) each time the MFC output stabilized across external loads. A control MFC (MFCcontrol) was made the same way and operated under the same conditions, but without addition of urine.  Both MFCs were operated for 40 days. The initial Open Circuit Voltage (OCV) of the MFC treated with urine (MFCurine) was 227mV and that of MFCcontrol was 219mV. Both MFCs   produced overlapping OCVs to the point of adding urine. The maximum OCVs of MFCcontrol and MFCurine prior to treatment were 729 mV and 740 mV respectively. The OCV of MFCurine increased to a maximum value of 755 mV, four days after the initial treatment. At the final stage (Day 40), OCV of MFCurine was 474.64mV; whereas the corresponding value for MFCcontrol was 7.31mV.  A micro chip was used to amplify the output of the MFCs to power a Light Emitting Diode. In addition, MFCurine was used to power a digital clock/thermometer. This study showed that human urine can be successfully utilized as fuel in a soil-based MSCMFC for the production of electrical energy which can be boosted to power low energy utility devices in farms or homes.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/4808
Editor: | International Commission of Agricultural and Biosystems Engineering

Relação:

http://www.cigrjournal.org/index.php/Ejounral/article/view/4808/2918

http://www.cigrjournal.org/index.php/Ejounral/article/downloadSuppFile/4808/2129

Formato: | application/pdf

Fonte:

Agricultural Engineering International: CIGR Journal; Vol 21, No 1 (2019): CIGR Journal; 115-121

1682-1130

Fonte: | Copyright (c) 2019 Agricultural Engineering International: CIGR Journal