Data/hora: 06/06/2024 05:41:31

Provedor de dados: 	111	
País: 	China	
Título: 	Alternative biomass furnace wall material from biomass furnace ash	
Autores: 	Flores, Edgar Dulay.	
Data: 	2017-06-12	
Ano: 	2017	
Palavras-chave: 	Biomass; Rice husk; Ash; Furnace; Mechanical dryer.	
Resumo: 	Biomass furnace ash (BFA) generated from drying of grains in mechanical dryers were blended with cement in varying ratio of 1:4, 1:5, 1:6, 1:7 and 1:8 by volume.  Each composition was cured in an ambient condition for 7, 14 and    28 days and determined their properties such as density, porosity, compressive strength and thermal shock resistance.  Cold crushing strength increased with increasing cement content and curing time.  Likewise, density increased with increasing cement content and curing time while porosity showed the other way.  All the sample compositions exceeded 30 cycles without any crack when subjected to thermal shock resistant cycles of heating and cooling using a firing temperature of 1000oC in an electric muffle furnace.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/3944	
Editor: 	International Commission of Agricultural and Biosystems Engineering	
Relação: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/3944/2533	
Formato: 	application/pdf	
Fonte: 	Agricultural Engineering International: CIGR Journal; Vol 19, No 1 (2017): CIGR Journal; 50-55

1682-1130	
Fonte: 	Copyright (c) 2017 Agricultural Engineering International: CIGR Journal