Data/hora: 09/06/2024 05:37:48

Provedor de dados: 	117	
País: 	Chile	
Título: 	A Rainfall Simulator for the in situ Study of Superficial Runoff and Soil Erosion	
Autores: 	Sangüesa,Claudia; Arumí,José; Pizarro,Roberto; Link,Oscar.	
Data: 	2010-03-01	
Ano: 	2010	
Palavras-chave: 	Soil erosion; Superficial runoff; Erosion plot; Uniformity of rain.	
Resumo: 	A rainfall simulator is an important tool for the study of runoff generation and soil loss because it can be used either under laboratory conditions, or in disturbed or natural soil. The objective of this study was to describe the design and operation of a rainfall simulator to evaluate soil loss in situ. The rainfall simulator has four full-cone spray nozzles with a Unijet system mounted in a straight line pipe configuration, and easily transported and assembled. Simulated rainfall uniformity was evaluated in the laboratory, whereas the applicability of the simulator in natural soil erosion plot conditions in an experimental field with different slopes was tested by quantifying runoff and evaluating soil erosion. Twenty simulations were carried out in the laboratory and sixteen in the field with slopes of 11, 21, and 39%. Four water-sprinklers in a straight line generated rainfall with uniformity close to 90%. The constructed simulator was easy to use and low cost, facilitating the necessary experimental replicates to achieve a suitable spatial representation of superficial runoff and soil loss on hillsides.	
Tipo: 	Journal article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0718-58392010000100019	
Editor: 	Instituto de Investigaciones Agropecuarias, INIA	
Formato: 	text/html	
Fonte: 	Chilean journal of agricultural research  v.70 n.1 2010