Data/hora: 11/06/2024 11:16:10

Provedor de dados: | 14
País: | Brazil
Título: | Procedimento para estimativa da intensidade de precipitação máxima admissível em pivô-central com base nas características do equipamento e do solo.
Autores: | RODRIGUES, L. N.; PRUSKI, F. F.; SILVA, E. M. da.
Data: | 2004-12-10
Ano: | 2003
Palavras-chave: | Escoamento superficial; Interceptação; Armazenamento superficial; Precision farming; Surface runoff; Infiltration water; Plant cover; Interception; Superficial storage.; Agricultura de Precisão; Água; Cobertura Vegetal; Infiltração; Irrigação; Pivô Central; Solo.; Agriculture; Irrigation; Soil; Water management.
Resumo: | ABSTRACT: A procedure to estimate the center pivot maximum application rate, based on equipment and soil characteristic is presented. It was developed to minimize the surface runoff. To achieve this objective, the Green and Ampt (GA) infiltration equation was modified to include surface sealing and surface storage. The highest application rate is determined by solving a system of equations which incout to application rate and its derivative and the GA and its derivative. Sensitivit analysis showed that the procedure represented adequately the variation in the main parameters that interfere in the value of the maximum application rate. This methodology can be used to desing the optimum center pivot irrigation system for given combination of soil, climate cropping pattern, and tillage practice. It can also be used to estimate the maximum aplication rate during irrigation for specific patches wthin the irrigated area
Tipo: | Documentos (INFOTECA-E)
Idioma: | Português

Identificador:

25012

http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/567998

Editor: | Planaltina, DF: Embrapa Cerrados, 2003.

Relação:

Embrapa Cerrados - Documentos (INFOTECA-E)

(Embrapa Cerrados. Documentos, 88).

Formato: | 53 p.