Data/hora: 04/06/2024 06:30:27

Provedor de dados: 	19	
País: 	Japan	
Título: 	ラグ3面用測定装置による外力測定と作用特性の検証

Force Measurements by Three-Surfaced Lug Type Transducers for Proving the Analysis of Soil Lug Interaction Characteristics	
Autores: 	岸本, 正; 大友, 功一; 趙, 誠瓚; 玉利, 達人; KISHIMOTO, Tadashi; OHTOMO, Koichi; CHO, Sung-Chan; TAMARI, Tatsuto.	
Data: 	2000-05	
Ano: 	2000	
Palavras-chave: 	農用車輪; ラグ; 推進力; 転がり抵抗; 接地荷重反力; Agricultural wheel; Lug; Traction; Motion resistance; Reaction to dynamic load.	
Resumo: 	農用車輪ラグの運動シミュレーションより得られた, ラグを構成する“前方ラグ面”,“外周ラグ面”および“後方ラグ面”の作用特性の解析結果を実験により検証した。これらの3面に作用する外力を測定するために, ラグ3面用小型トランスデューサを供試して法線方向力と接線方向力を各面別に独立して測定し, この2分力から車輪回転角や供試ラグの角度要素を用いて各面に作用する推進力, 転がり抵抗, 接地荷重反力を求めた。この結果, 前方ラグ面は転がり抵抗と接地荷重反力, 外周ラグ面は転がり抵抗, 接地荷重反力さらに推進力, また, 後方ラグ面は推進力と接地荷重反力を発生しており, 運動解析より得られた結果と一致した。 This research proves the results of the motion analyses of interactions between soil and wheel lug surfaces. Normal and tangential forces acting on the surfaces were measured by small-sized transducers of three-surfaced lug type，and the traction，the motion resistance and the reaction to the dynamic load were calculated with wheel rotational and lug design angles. The results of experiments indicated that (1) the trailing lug side produced the motion resistance and the reaction to the dynamic load，(2 ) the lug face produced the motion resistance，the traction and the reaction to the dynamic load，and (3) the leading lug side produced the traction and the reaction to the dynamic load. These were in accordance with the results of wheel motion analysis.	
Idioma: 	Japonês	
Identificador: 	http://ir.obihiro.ac.jp/dspace/handle/10322/2956	
Editor: 	農業機械学会	
Formato: 	application/pdf	
Fonte: 	農業機械学会