Data/hora: 18/06/2024 12:11:46

Provedor de dados: 	20	
País: 	Belgium	
Título: 	Características de la red de cerco "tipo lámpara" y algunos comentarios sobre la flota que la utiliza en la pesca de caballa.

Characteristic of the lampara net used in mackerel fishing and some comments about the fleet	
Autores: 	Izzo, A.; Boccanfuso, J.	
Data: 	2008-07-19	
Ano: 	1993	
Palavras-chave: 	Buoyancy floats; Fishing effort; Surface temperature; Ballast; Fishing effort; Fishing effort; Fishing effort; Http://aims.fao.org/aos/agrovoc/c_24027; Http://aims.fao.org/aos/agrovoc/c_24027.	
Resumo: 	The composition of the fleet is analyzed. The boats range 50-200 HP of engine and have 9-16 m in length overall. Most of the boats have been improving their equipment (echosounders, new engines) since 1980. An inverse relationship was found between sea surface temperature and CPUE as measured by mackerel catch permit time spent on fishing gounds. Yields are negligible over 20°C with a optimum of 20°C.	
Tipo: 	Journal Contribution	
Idioma: 	Espanhol	
Identificador: 	INIDEP documento científico, 2. p. 45-52

0327-9332

http://hdl.handle.net/1834/2573	
Editor: 	Mar del Plata: Instituto Nacional de Investigación y Desarrollo Pesquero