Data/hora: 08/06/2024 18:22:06

Provedor de dados: | 20
País: | Belgium
Título: | Influence of Seawall Line Choice on Tide Lock Drainage in Tidal Flat Inning:Cangdongpian Inning Area on the west part of Tiaozini Sand as a case study.
Autores: | Li, Jialin; Wang, Yanhong; Zhang, Renshun.
Data: | 2015-01-21
Ano: | 2007
Palavras-chave: | Tidal flats; River discharge.
Resumo: | Most of the flood from the wide inner lowland plain discharges through tide locks on coast, and the influence of tidal flat inning projects on the tide lock drainage must be solved by seawall line choice. Taking the Cangdongpian inning area on the west side of Tiaozini Sand as a case study, the paper analyzed the compages and validity of ebb tide water to maintain the flood discharge creek below the tide lock for different projects of seawall line. Result indicates that a rational seawall line program has little influence on the flood discharge of lock during the mean tide or general spring tides, but has certain influences during a storm surge or an extreme spring tide in autumn. However it could be resolved by several times of artificial scour on the creek.
Tipo: | Journal Contribution
Idioma: | Inglês

Identificador:

Marine Science Bulletin, 9 (1), 55-65

1000-9620

http://hdl.handle.net/1834/5854

Fonte: | http://creativecommons.org/licenses/by-nc/3.0/