Data/hora: 08/06/2024 12:43:54

Provedor de dados: | 27
País: | Belgium
Título: | An automated method for the assessment of mercury adsorption rates on particulate suspended matter
Autores: | Baeyens, W.F.J.; Decadt, G.; Dehairs, F.A.; Goeyens, L.
Data: | 1982
Ano: | 1982
Palavras-chave: | Adsorption; Mercury; Methodology; Particulates; Suspended matter.
Resumo: | A continuous filtration system connected to a mercury auto-analyzer has been constructed for obtaining mercury adsorption rates on particulate suspended matter. The capabilities of this device have been demonstrated by carrying out a series of experiments under controlled physicochemical parameter conditions on samples of the Scheldt estuary. Duplicate measurements showed coefficients of variation ranging from 1 to 6 %. Depending on the physico-chemical conditions, the initial adsorption rate per unit of dissolved mercury concentration varied between 1.2 and 8.1 x 10&lt;sup&gt;-2&lt;/sup&gt; mn&lt;sup&gt;-1&lt;/sup&gt;.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.vliz.be/nl/open-marien-archief?module=ref&refid=3413
Relação: | info:eu-repo/semantics/altIdentifier/wos/A1982PA49500001
Fonte: | %3Ci%3EOceanol.+Acta+5%283%29%3C%2Fi%3E%3A+261-264
Fonte: | info:eu-repo/semantics/restrictedAccess