Data/hora: 09/06/2024 07:47:36

Provedor de dados: 	27	
País: 	Belgium	
Título: 	An automated method for the assessment of mercury adsorption rates on particulate suspended matter	
Autores: 	Baeyens, W.F.J.; Decadt, G.; Dehairs, F.A.; Goeyens, L.	
Data: 	1982	
Ano: 	1982	
Palavras-chave: 	Adsorption; Mercury; Methodology; Particulates; Suspended matter.	
Resumo: 	A continuous filtration system connected to a mercury auto-analyzer has been constructed for obtaining mercury adsorption rates on particulate suspended matter. The capabilities of this device have been demonstrated by carrying out a series of experiments under controlled physicochemical parameter conditions on samples of the Scheldt estuary. Duplicate measurements showed coefficients of variation ranging from 1 to 6 %. Depending on the physico-chemical conditions, the initial adsorption rate per unit of dissolved mercury concentration varied between 1.2 and 8.1 x 10&lt;sup&gt;-2&lt;/sup&gt; mn&lt;sup&gt;-1&lt;/sup&gt;.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.vliz.be/nl/open-marien-archief?module=ref&refid=3413	
Relação: 	info:eu-repo/semantics/altIdentifier/wos/A1982PA49500001	
Fonte: 	%3Ci%3EOceanol.+Acta+5%283%29%3C%2Fi%3E%3A+261-264	
Fonte: 	info:eu-repo/semantics/restrictedAccess