Data/hora: 08/06/2024 11:46:51

Provedor de dados: 	27	
País: 	Belgium	
Título: 	The Tertiary and Quaternary subbottom of the Schelde estuary near Antwerpen (Belgium)	
Autores: 	Wartel, S.	
Data: 	1980	
Ano: 	1980	
Palavras-chave: 	Estuaries Quaternary River beds Tertiary Belgium; Zeeschelde.	
Resumo: 	The subbottom stratigraphy of the Schelde estuary near Antwerpen was studied using an ORE subbottom profiler. The estuary valley is incised in Tertiary and Quaternary deposits, still eroded at several places. In the Boom Clay (Oligocene) uparching and diapers occur. They result from an unloading erosion surface, dipping roughly NNE and covered unconformably by Miocene (Edegem Sands) and Pliocene (Kattendijk Sands) deposits. The contact between Miocene and Pliocene has not been observed. The lowermost Quaternary deposit consists of a gravel and shell layer irregular in thickness and unconformable with the older deposits. The recent sediment cover, where present, is less than 1 m thick.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.vliz.be/nl/open-marien-archief?module=ref&refid=3704	
Fonte: 	%3Ci%3EGeol.+Mijnbouw+59%283%29%3C%2Fi%3E%3A+233-240	
Fonte: 	info:eu-repo/semantics/restrictedAccess