Data/hora: 01/06/2024 02:47:25

Provedor de dados: 	32	
País: 	Mexico	
Título: 	Análisis de las unidades de riego con aprovechamiento superficial en la Cuenca Lerma Chapala, México.	
Autores: 	González Covarrubias, Galdino Daniel.	
Data: 	2013-10-22	
Ano: 	2013	
Palavras-chave: 	Modelación; SIG; Riego; Agua; Sustentabilidad; Cuenca; Modeling; GIS; Irrigation; Water; Sustainability; Watershed; Hidrociencias; Maestría Tecnológica.	
Resumo: 	En el presente estudio se realizó el análisis de las Unidades de Riego con aprovechamiento superficial en la Cuenca Lerma Chapala, México, a través de la georrefenciación y caracterización de la infraestructura hidroagrícola, padrón de usuarios y catastro, integrándolos en un Modelo de Sistema de Información Geográfica (SIG). Esto permitió conocer en forma precisa la información relevante de dichas Unidades. Se caracterizaron 1,364 unidades de riego con un total de 56,266 usuarios que detentan 114,975.26 hectáreas. La longitud de la red de conducción es de 2,435 km y la longitud de la red de drenaje es de 2,643 km, y 34,965 estructuras de control.  La integración de las capas de información generadas en formato shape-file (*.shp) al Modelo de SIG de la Cuenca Lerma Chapala, permite tener herramientas valiosas de apoyo en la toma de decisiones para el correcto direccionamientos de las acciones estructurales y no estructurales para lograr el uso sustentable del agua en esta cuenca. Más del 90% de los usuarios de las Unidades de Riego con fuente de agua superficial optan por asegurar cultivos de Primavera-Verano con una lámina de riego reducida en comparación a la requerida en cultivos de Otoño-Invierno. El patrón de cultivos se integra fundamentalmente por maíz (70.79%), sorgo (10.25%) y trigo (8.34%). El Modelo de SIG de la Cuenca Lerma Chapala, permitirá, a través del uso de imágenes de satélite, cuantificar en forma precisa la superficie cultivada a nivel de parcela y estimar en forma indirecta el uso de agua para riego. _______________ ABSTRACT: In the present study carried out in the Irrigation Units of the Lerma-Chapala (Mexico) Watershed, the analysis of the surface water use was performed by georeferencing and characterizing hydro infrastructure, users and crops. This information gathered in shape-files was integrated in a Geographic Information System (GIS) Model in order to know and analyze in accurate way the relevant information of such irrigation units. There were characterized 1,364 irrigation units with 56,266 users owning 114,975.26 ha. The length of the water conduction net is 2,435 km and the length of the drainage net is 2,643 km. There were identified 34, 965 structures to control the water flow. The GIS Model is a valuable tool for decision makers to support the design and direction of structural and no-structural actions aimed to reach the water use sustainability in the study area. More than 90% of the producers use surface water to irrigate spring-summer crops with less volume compared to that required in autumn-winter crops. In terms of seeded area in the irrigation units, the main crops are corn (70.79%), sorghum (10.25%) and wheat (8.34%). By using updated satellite images, the GIS Model developed for the Lerma-Chapala (Mexico) Watershed will permit to measure the cropped area and estimate the water volume for irrigation by crop at different levels (watershed, irrigation unit and lot).	
Idioma: 	Espanhol	
Identificador: 	http://hdl.handle.net/10521/2072