Data/hora: 02/06/2024 18:39:49

Provedor de dados: | 32
País: | Mexico
Título: | Alcances y limitaciones de la información espectral multi-angular para la clasificación de la vegetación
Autores: | Cano González, Alejandro de Jesús.
Data: | 2012-09-08
Ano: | 2008
Palavras-chave: | Clasificación; Información espectral muti-angular; Sensores remotos; CCRF; Doctorado; Hidrociencias; Classification; Multi angular spectral information; Remote sensing.
Resumo: | El uso de información espectral multi-angular se ha justificado como una estrategia  para aumentar la precisión de los sistemas de clasificación de cultivos y vegetación  natural. En este trabajo se discuten los esquemas de caracterización de la  información espectral multi-angular asociada a la vegetación, así como su uso en los  sistemas de clasificación. Los resultados mostraron que, dejando fijo el fondo de la  vegetación, es posible discriminar sistemas arbolados y, cuando el fondo de la  vegetación varía, existe confusión con coberturas aéreas bajas. Por lo tanto, se  planteo un segundo experimento, presentando un modelo de los efectos del ángulo  cenital de visión e iluminación en las reflectancias bi-cónicas (Conical-Conical  Reflectance Factor, CCRF) de especies vegetales contrastantes y suelo desnudo.  Los resultados analizados para el efecto del suelo y la densidad de plantas muestran  que hay importantes zonas de confusión (traslape de información) entre las especies,  al considerar efectos combinados, para diversas diferencias acimutales. Estos  resultados ponen en duda el uso en forma generalizada de la información espectral  multi-angular y solo justifican este enfoque de clasificación si se dejan fijos el fondo  de la vegetación y la densidad de plantas (cantidad de follaje), situación irreal en un  sistema operacional. Debido a esto se presentó un esquema de modelación global  de los ángulos cenitales y acimutales en la reflectancia de la vegetación, extendiendo  los desarrollos al caso de los efectos de cambios en las propiedades ópticas del  fondo de la vegetación (suelos) y de la densidad de plantas (follaje), ratificándose el  problema de confusión en la discriminación de especies. Para poder concluir de  manera definitiva sobre el uso de la información multi-angular, se recomienda  realizar otro tipo de modelaciones, relacionando los parámetros B y las reflectancias  a nadir y el efecto multi-angular en las curvas iso-IAF. _____________The use of multi-angular spectral information has been justified like a strategy to  increase the precision of vegetation classification systems. In this work the schemes  of characterization of the multi-angular spectral information associated to the  vegetation, as well as its use in the classification systems are discussed. The results  showed that leaving the bottom of the vegetation unchanging, it is possible to  discriminate tree systems and, when the bottom of the vegetation varies, exist  confusion with low aerial covers. Therefore, a second experiment was considered to  analyze the discrimination of the vegetation under different approaches of  characterization, being presented a model of the effects of the zenithal angle of vision  and illumination in biconical reflectances (Conical-Conical Reflectance Factor, CCRF)  of contrast vegetal species and bare soil. The results analyzed for the effect of the  ground and the density of plants show that there are important zones of confusion  (overlaps of information) between the species, when considering combined effects,  for diverse azimuth differences. These results put in doubt the use in a generalized  form of the multi-angular spectral information and only justify its use if the bottom of  the vegetation and the density of plants (amount of foliage) are left unchanging,  unreal situation in an operational system. Due to this a scheme of global modeling of  the zenith and azimuth angles in the reflectance of the vegetation appeared,  extending the developments to the case of changes in the optical properties of the  bottom of the vegetation (grounds) and the density of plants (foliage), ratifying the  problem of confusion in the discrimination of species. In order to be able to conclude  in a definitive way on the use of the multi-angular information, it is recommended to  make another type of modeling,   relating  B parameters and nadir reflectance’s  and  the multi-angular effect in the iso-IAF curves.
Tipo: | Tesis
Idioma: | Espanhol
Identificador: | http://hdl.handle.net/10521/1240