Data/hora: 01/06/2024 07:47:05

Provedor de dados: | 32
País: | Mexico
Título: | Factibilidad económica para el aprovechamiento de aguas tratadas de PTAR Atapaneo en módulos II al IV del DR020 Morelia-Queréndaro utilizando SIG.
Autores: | Gaona Quesada, Rafael.
Data: | 2013-10-21
Ano: | 2013
Palavras-chave: | Aguas residuales; Diseño hidráulico; Indicadores económicos; Wastewater; Hydraulic design; Economic indicators; Hidrociencias; Maestría Tecnológica.
Resumo: | Existe una planta de tratamiento de aguas residuales (PTAR) en el río Grande de Morelia que tiene una capacidad para 2.19 m3s-1, cuya agua tratada se mezcla con el agua del río proveniente de la presa y luego se conduce para irrigar las superficies de los módulos II, III y IV del Distrito de Riego 020 Morelia-Queréndaro, Michoacán. Los usuarios de estos módulos, tienen concesión para usar tanto el agua del río proveniente de la presa así como para usar el agua residual de la ciudad de Morelia. En este trabajo se evalúa la factibilidad económica de entubar el agua proveniente de la PTAR y llevarla hasta el punto de control de cada uno de los módulos. Con el proyecto se podrá evitar la mezcla de aguas residuales con agua proveniente de la presa y de tener menos pérdidas por evaporación e infiltración en la conducción, además tendría un beneficio adicional en la oportunidad del riego. Después de recopilar información, se realizó una propuesta de trazo para la conducción sobre el sistema de información geográfica del distrito de riego. Luego se identificaron los costos y los beneficios del proyecto, basados en un diseño hidráulico de la tubería principal, y se realizó una evaluación económica donde se obtuvieron indicadores de R B/C = 1.41, VPN= 71,795y TIR=16.5%. Finalmente se concluye que si es factible entubar el tramo de conducción desde la PTAR hasta la zona de riego de los módulos II, III y IV y es económicamente redituable. _______________ ECONOMICAL FEASIBILITY FOR THE USE OF TREATED WATER WWTP ATAPANEO ON MODULES II TO IV OF DR-020 MORELIA-QUERENDARO USING GIS. ABSTRACT: There is a waste water treatment plant (WWTP) on the “Grande de Morelia” river which has a capacity of 2.19 m3 s-1, whose treated water is mixed with river water from the dam and then it leads to irrigate surfaces on modules II, III and IV of the Irrigation District 020 Morelia-Queréndaro, Michoacán. Users of such modules are granted to use both river water from the dam and to use wastewater from the city of Morelia. Currently the treated water mixes with river water from the dam and then it is ducted to flush the surfaces of downstream modules. This paper evaluates the economic feasibility of piping water from the WWTP and taking it to the handle of each of the modules. The project will prevent mixing sewage water and water from the dam and have less evaporation and infiltration losses in its conduction; it would also have an additional benefit in the timing of irrigation. After gathering information, a proposal was made for conduction line on the geographic information system of the irrigation district. There were identified the costs and benefits of the project, based on a main pipe hydraulic design, and performed an economic evaluation  whose indicators are B / C R = 1.41, NPV=71,795and IRR = 16.5%. Finally, it is concluded that it is possible to pipe the conducting section from the WWTP to the irrigation module II, III and IV, and it is economically profitable.
Idioma: | Espanhol
Identificador: | http://hdl.handle.net/10521/2067