Data/hora: 13/06/2024 06:02:23

Provedor de dados: | 32
País: | Mexico
Título: | Prototipo de un penetrómetro cónico de impacto y su validación de uso en suelos forestales
Autores: | Vásquez García, Irma.
Data: | 2010-05-14
Ano: | 2010
Palavras-chave: | Resistencia mecánica; Penetrómetro cónico; Física de suelos; Suelo forestal; Densidad aparente; Soil strength; Conic penetrometer; Soil physics; Forest soils; Bulk density; Maestría; Forestal.
Resumo: | La resistencia mecánica del suelo es un indicador importante de su condición física. Dado que en el Inventario Forestal y de Suelos de México se requiere incluir indicadores de la condición física del suelo, en el presente estudio se diseñó y validó un penetrómetro cónico dinámico para medir la resistencia mecánica de suelos forestales. El diseño del equipo tiene la ventaja de ser ligero, portátil y práctico. Para la validación se hicieron pruebas de campo en diferentes ecosistemas y se emplearon en laboratorio cuatro tipos de suelos (Calcisol, Leptosol, Feozem y Andosol). Se encontró que una serie de 10 impactos genera mediciones independientes y confiables sobre la resistencia mecánica del suelo superficial. La aportación de este trabajo demuestra que con principios técnicos es posible adecuar implementos de campo para la valoración de la condición física del suelo, sin tener que depender de tecnología importada, que frecuentemente es costosa. _______________(Prototype of a impact conic penetrometer and their use in  forest soils validation). ABSTRACT : Soil strength is an important indicator of soil physical conditions. Because the Forest and Soils Inventory of Mexico is requiring to include indicators of soil physical condition, a dynamic cone penetrometer for measuring soil strength in forest soils was designed and validated in this study. The designed penetrometer has the advantage of being lightweight, portable and of practical use. To validate the penetrometer, field measurements were made under different ecosystems and in laboratory, using four types of soils (Calcisol, Leptosol, Phaeozem and Andosol). Results shows that a series of 10 impacts generates independent and reliable measurements of soil strength on the soil surface. This work confirms that using basic technical principles, a useful field tool for assessing soil physical conditions can be built without relying on imported technology, which is often costly.
Idioma: | Espanhol
Identificador: | http://hdl.handle.net/10521/87