Data/hora: 15/06/2024 11:27:30

Provedor de dados: | 32
País: | Mexico
Título: | Caracterización morfométrica y simulación del balance de la cuencia "Tres Valles, S. L.P.".
Autores: | Sánchez Orta, Santiago.
Data: | 2010-08-27
Ano: | 2010
Palavras-chave: | Balance hidrológico; Producción de agua; Modelo hidrológico; Modelo SWAT; Hydrological balance sheet; Water production; Hydrological model; Model SWAT; Maestría; Hidrociencias.
Resumo: | En la actualidad la escasez de agua es un problema que ha inducido a la realización de estudios hidrológicos a nivel mundial, el uso de los sistemas computacionales e informáticos son herramientas muy importantes para la agilización de los estudios. En el caso del presente estudio, se a empleado un Sistema de Información Geográfica, en el cual se realizó la simulación del balance hidrológico de la Cuenca Tres Valles de los estados de San Luis Potosí y Tamaulipas en el año 2007, aplicando el modelo hidrológico SWAT, esto con la finalidad de obtener de manera rápida y precisa la distribución de los diversos fenómenos hídricos que se presentan al interior de una cuenca. Dicha simulación se plantea como una alternativa para evaluar la cantidad de agua total en cuencas, donde hay nula o escasa infraestructura de medición de caudales. El periodo simulado fue de 1989 a 2007, la calibración del modelo nos proporciono un coeficiente de determinación de R2= 0.840 el cual nos permitió obtener un volumen total de 4,599.611 Mm3/año, con una precipitación media de 1,161.94 mm, dentro de la cuenca. La producción anual de agua simulada fue de una lamina de 736.64 mm, lo que genero un volumen de 2,916.071 Mm3/año. Teniendo una disponibilidad total de agua en  abstracciones hidrológicas y utilización en diferentes sectores de 1,683.597 Mm3/año, en una superficie total de 395,861.164 ha. _______________ MORPHOMETRIC CHARACTERIZATION AND SIMULATION OF THE STOCK OF THE THREE VALLES WATERSHED, SAN LUIS POTOSI. ABSTRACT: At present, water shortage is a problem that has led the hydrological studies worldwide, the use of computer and computer systems are very important tools for the improvement of studies.  In the case of this study was to use a Geographic Information System, which was carried out simulation of catchment water balance of the Three Valleys of the states of San Luis  Potosi and Tamaulipas in 2007, using the SWAT hydrological model, this in order to obtain quick and accurate distribution of the different phenomena occurring water within a watershed. This simulation is proposed as an alternative to evaluate the amount of water in basins, where there is little or no flow measurement infrastructure. The simulated period was 1989-2007, the calibration of the model provided us with a determination coefficient of R2 = 0.840 which allowed us to obtain a total volume of 4599.611 Mm3/year, with an average rainfall of 1161.94 mm, within the watershed. The annual water production was simulated with a layer of 736.64 mm, which generated a volume of 2916.071 Mm3/year. Having a total availability of water in hydrological abstractions and utilization in different sectors of 1,683.597 Mm3/año, in a total surface of 395,861.164 it has.
Idioma: | Espanhol
Identificador: | http://hdl.handle.net/10521/160