Data/hora: 05/06/2024 13:59:48

Provedor de dados: | 45
País: | Brazil
Título: | Silage of rehydrated corn grain
Autores: | Mombach,M.A.; Pereira,D.H.; Pina,D.S.; Bolson,D.C; Pedreira,B.C.
Data: | 2019-06-01
Ano: | 2019
Palavras-chave: | Water; Concentrate; Ensiling; Fermentation; Moisture.
Resumo: | ABSTRACT The objective with this study was to evaluate the effect of different levels of water inclusion on the chemical composition and fermentation profiles of reconstituted corn grain silage. The experiment was carried out in a factorial arrangement in a completely randomized design, with three replicates per treatment. Five treatments were evaluated with different levels of water inclusion (% of the natural matter): dry corn grain (control); 90% dry corn grain (DCG) and 10% water; 80% DCG and 20% water; 70% DGC and 30% water; and 60% DCG and 40% water, totaling 45 experimental silos. Inclusion of water in the silage of reconstituted corn grain promoted a reduction in the CP (%) and NDF (%) contents. However, the water increase elevated the NPN/TN contents and the amount of effluent, gas and dry matter (%) losses. The treatment with inclusion of 30% water in the natural matter leads to a better fermentation profile and fewer losses of effluent and dry matter, so it is recommended for ensiling dry ground corn grain.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0102-09352019000300959
Editor: | Universidade Federal de Minas Gerais, Escola de Veterinária
Relação: | 10.1590/1678-4162-9676
Formato: | text/html
Fonte: | Arquivo Brasileiro de Medicina Veterinária e Zootecnia  v.71 n.3 2019
Fonte: | info:eu-repo/semantics/openAccess