Data/hora: 01/06/2024 14:24:25

Provedor de dados: | 5
País: | France
Título: | Copolarized and Cross‐Polarized SAR Measurements for High‐Resolution Description of Major Hurricane Wind Structures: Application to Irma Category 5 Hurricane
Autores: | Mouche, Alexis; Chapron, Bertrand; Knaff, John; Zhao, Yili; Zhang, Biao; Combot, Clement.
Data: | 2019-06
Ano: | 2019
Palavras-chave: | SAR; Copolarization and cross-polarization; High resolution; Category 5 Hurricane; Hurricane Irma.
Resumo: | C‐Band high resolution radar (SAR) is the only space‐borne instrument able to probe at very high resolution and over all ocean basins the sea surface under extreme weather conditions. When co‐analyzed with Stepped Frequency Microwave Radiometer (SFMR) wind estimates, the radar backscatter signals acquired in major Hurricanes from Sentinel‐1 and Radarsat‐2 SAR, reveal high sensitivity in the cross‐polarized channel for wind speeds up to 75 m/s. The combination of the two co‐ and cross‐ polarized channels can then be used to derive high resolution surface wind estimates. The retrieval methods and impacts of intense rainfall are discussed in the context of a Hurricane Irma (2017) case study. On September 7, 2017, Sentinel‐1 measurements intercepted Hurricane Irma when it was at category 5 intensity. When compared to SFMR, SAR‐derived wind speeds yield bias and rms, of about 1.5 m/s and 5.0 m/s, respectively. The retrieved wind structure parameters for the outer core are found to be in agreement with the Best‐Track and combined satellite and aircraft based analyses. SAR measurements uniquely describe the inner core and provide independent measurements of the maximum wind speed, the radius of maximum wind (RMW). Near the RMW a 65 m/s increase in wind speed in less than 10 km is detected, corresponding to an instantaneous absolute vorticity of order 210 times the Coriolis parameter. Using a parametric Holland model and the environmental surface pressure (1011 hPa), SAR‐derived wind speeds correspond to a central surface pressure of 918 hPa (921 hPa from the Best‐Track) in Irma's eye.
Tipo: | Text
Idioma: | Inglês

Identificador:

https://archimer.ifremer.fr/doc/00497/60898/64236.pdf

DOI:10.1029/2019JC015056

https://archimer.ifremer.fr/doc/00497/60898/

Editor: | American Geophysical Union (AGU)
Formato: | application/pdf
Fonte: | Journal Of Geophysical Research-oceans (2169-9275) (American Geophysical Union (AGU)), 2019-06 , Vol. 124 , N. 6 , P. 3905-3922

Fonte:

info:eu-repo/semantics/openAccess

restricted use