Data/hora: 13/06/2024 08:56:27

Provedor de dados: | 5
País: | France
Título: | Very High Resolution 3D seismic: a new imaging tool for sub-bottom profiling
Autores: | Marsset, Tania; Marsset, Bruno; Thomas, Yannick; Didailler, Stephane.
Data: | 2002-05
Ano: | 2002
Palavras-chave: | Imagery; 3D; VHR; Seismic; Imagerie; 3D; THR; Sismique.
Resumo: | This note presents the first results of the development of a 3D Very High Resolution seismic method. Particular attention was paid to the design of an operational system to be in agreement with the expected goals in term of acquisition and processing. A set of three examples, collected in various geological environments, is presented.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/2002/publication-495.pdf

http://archimer.ifremer.fr/doc/2002/sup-495.pdf

DOI:10.1016/S1631-0713(02)01766-2

Editor: | Elsevier
Relação: | http://archimer.ifremer.fr/doc/00000/495/
Formato: | application/pdf
Fonte: | Comptes Rendus Geoscience (1631-0713) (Elsevier), 2002-05 , Vol. 334 , N. 6 , P. 403-408
Fonte: | 2002 Académie des sciences / Éditions scientifiques et médicales Elsevier SAS. All rights reserved.