Data/hora: 15/06/2024 03:07:45

Provedor de dados: | 5
País: | France
Título: | Delayed mode quality control of Ovide Argo Data. Float WMO 6900399
Autores: | Lagadec, Catherine; Thierry, Virginie; Cabanes, Cecile.
Data: | 2015-10-29
Ano: | 2015
Resumo: | This report presents the delayed mode analysis of an Argo float. Real time quality control flags are checked and interesting profiles are plotted.  The OW method (objective analysis) is used to detect a conductivity sensor drift and correct it, if any.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00311/42193/41508.pdf

http://archimer.ifremer.fr/doc/00311/42193/

Formato: | application/pdf

Fonte:

2015 Ifremer

info:eu-repo/semantics/openAccess

restricted use