Data/hora: 03/06/2024 10:55:21

Provedor de dados: 	5	
País: 	France	
Título: 	Testing the effectiveness of tough resin systems for improving structural performance of joints in GRP ships.	
Autores: 	Norwood, L; Caulier, C.	
Data: 	1992-12	
Ano: 	1992	
Palavras-chave: 	Ships; Adhesion; Joints; Shear; Ship technology; Glass reinforced plastics; Materials testing; Composite materials; Urethane acrylate; Raidisseur; Coque; Fixation; Joint.	
Resumo: 	A major concern in any composite structure is its ability to resist peel and shear loading; this becomes a more difficult problem where long delays in laminating have occurred or when dissimilar materials are joined together. In the case of mine countermeasure vessels, adhesion between stiffener and hull becomes critical when the ship is subjected to underwater shock loading. In order to reduce costs and improve the hull-stiffener bond, tough resin systems based on urethane acrylates have been developed to replace the mechanical crack-stopping system currently employed. This paper describes the benefits of urethane acrylates in the frame-hull application discussing the level of improvement over the mechanical system.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/1992/acte-1043.pdf	
Editor: 	Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1992	
Relação: 	http://archimer.ifremer.fr/doc/00000/1043/	
Formato: 	application/pdf