Data/hora: 13/06/2024 04:58:36

Provedor de dados: 	5	
País: 	France	
Título: 	Le comportement en fluage, en fatigue et la tenue au feu de composites sandwichs	
Autores: 	Chevalier, J.	
Data: 	1992-12	
Ano: 	1992	
Palavras-chave: 	Fatigue (materials); Creep; Fire; Ship technology; Ship design; Composite materials; Feu; Nid d'abeille; PVC; Ame balsa; Sandwich; Composite.	
Resumo: 	Baltek Corp. is currently in the process of introducing 3 new products: density select material, AL-600/10 and DecoLite panels, that reduce weight and cost. Creep results on typical core materials have shown that only end-grain balsa (EGB) and 9.0 lb. Nomex honeycomb were capable of continuous operation at 160 F (71 degree C). In reverse bending fatigue studies, EGB has a fatigue limit 2-2.4 times that of the PVC foams. Finally, while EGB by itself is a ASTM E-84 Class 2 material, with the proper skins and resin system, it can easily meet Class 1 requirements.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/1992/acte-1065.pdf	
Editor: 	Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1992	
Relação: 	http://archimer.ifremer.fr/doc/00000/1065/	
Formato: 	application/pdf