Data/hora: 10/06/2024 18:46:34

Provedor de dados: 	5	
País: 	France	
Título: 	Lorient Flume tank	
Autores: 	Vincent, Benoit; Simon, Julien; Vacherot, Jean-philippe; Morandeau, Fabien; Larnaud, Pascal; Kopp, Dorothee; Mehault, Sonia; Morfin, Marie; Savina-rolland, Marie; Marc, Emilie.	
Data: 	2018-04-20	
Ano: 	2018	
Resumo: 	The Lorient flume tank is an hydrodynamic facility available for any qualification and observation of submerged objects in still or moving water. It is a closed loop circulating tank filled with fresh water.  The fluid is moved with a 70 kW pump-motor with a velocity between 0 and 1 m/s and homogenized with a series of pressure drop systems. The overall dimensions are 24.50 m long, 7.50m wide and 3.30 m high. The part where experiments can be set up is 12m long, 2.6 m wide and 1.5 m deep.  A mobile bottom belt can be synchronized with the water flow velocity and enables to simulate the seabed velocity relatively to a towed object. The overall process of the facility is controlled by a user friendly interface.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00436/54803/56299.pdf

DOI:10.13155/54803

http://archimer.ifremer.fr/doc/00436/54803/	
Formato: 	application/pdf	
Fonte: 	2018 Ifremer

info:eu-repo/semantics/openAccess

restricted use